PROTEL NETLIST 2.0
[
DESIGNATOR
U2
FOOTPRINT
SOT-89_L4.5-W2.5-P1.50-LS4.2-BR
PARTTYPE
ME6211A33PG-N
DESCRIPTION
输出极性:正极;工作电压:6V;输出电压:3.3V;输出电流:500mA;电源纹波抑制比(PSRR):70dB@(1kHz);输出类型:固定;
Component Kind
Standard
Add into BOM
yes
Convert to PCB
yes
Symbol
ME6211A33PG-N
Designator
U2
Device
ME6211A33PG-N
Unique ID
gge1
Name
ME6211A33PG-N
Reuse Block

Group ID

Channel ID

LCSC Part Name
3.3V 500mA 6V
Supplier Part
C236673
Manufacturer
MICRONE(南京微盟)
Manufacturer Part
ME6211A33PG-N
Supplier Footprint
SOT-89
JLCPCB Part Class
Extended Part
Datasheet
https://item.szlcsc.com/datasheet/ME6211A33PG-N/236113.html
Supplier
LCSC
3D Model Title
SOT-89-3_L4.3-W2.5-H1.6-LS4.1-P1.50
Output Configuration
正极
Voltage - Supply
6V
Output Voltage
3.3V
Output Current
500mA
Power Supply Rejection Ratio (PSRR)
70dB@(1kHz)
Voltage Dropout
120mV@(100mA)
standby current
30uA
Noise
50uVrms
Features
使能控制；短路保护；过流保护
Operating Temperature
-40℃~+150℃@(Ta)
Output Type
固定
Number of Outputs
1
Description
输出极性:正极;工作电压:6V;输出电压:3.3V;输出电流:500mA;电源纹波抑制比(PSRR):70dB@(1kHz);输出类型:固定;

*
]
[
DESIGNATOR
U5
FOOTPRINT
LGA-16_L3.0-W3.0-P0.50-TL
PARTTYPE
LIS3DHTR
DESCRIPTION
传感器类型:加速度计;接口类型:I2C；SPI;
Component Kind
Standard
Add into BOM
yes
Convert to PCB
yes
Symbol
LIS3DHTR_C15134
Designator
U5
Device
LIS3DHTR
Unique ID
gge4
Name
LIS3DHTR
Reuse Block

Group ID

Channel ID

LCSC Part Name
MEMS数字输出运动传感器：超低功耗、高性能三轴加速度计
Supplier Part
C15134
Manufacturer
ST(意法半导体)
Manufacturer Part
LIS3DHTR
Supplier Footprint
LGA-16(3x3)
JLCPCB Part Class
Extended Part
Datasheet
https://item.szlcsc.com/datasheet/LIS3DHTR/15808.html
Supplier
LCSC
3D Model Title
LGA-16_L3.0-W3.0-P0.50-TL
Accelerometer Sensing Axis
X,Y,Z
Acceleration Measurement Range (MAX)
±16g
Gyroscope Sensing Axis
-
Gyroscope Measurement Range (MAX)
-
Sensor Type
加速度计
Output Bits
16bit
Interface
I2C；SPI
Voltage - Supply
1.71V~3.6V
Cache Size
-
Standby Current
500nA
Operating Temperature
-40℃~+85℃
Features
运动事件检测
Description
传感器类型:加速度计;接口类型:I2C；SPI;

*
]
[
DESIGNATOR
U3
FOOTPRINT
TQFN-16_L3.0-W3.0-P0.50-BL-EP1.5
PARTTYPE
MAX98357AETE+T
DESCRIPTION
功放类型:D类功放;扬声器通道数:-;输出功率:3.2W×1@4Ω;静态电流(Iq):2.4mA;
Component Kind
Standard
Add into BOM
yes
Convert to PCB
yes
Symbol
MAX98357AETE+T
Designator
U3
Device
MAX98357AETE+T
Unique ID
gge23
Name
MAX98357AETE+T
Reuse Block

Group ID

Channel ID

LCSC Part Name
微型、低成本、PCM 类 D 级放大器具有 AB 级性能
Supplier Part
C910544
Manufacturer
ADI(亚德诺)/MAXIM(美信)
Manufacturer Part
MAX98357AETE+T
Supplier Footprint
TQFN-16-EP(3x3)
JLCPCB Part Class
Extended Part
Datasheet
https://item.szlcsc.com/datasheet/MAX98357AETE%252BT/978950.html
Supplier
LCSC
3D Model Title
TQFN-16_L3.0-W3.0-P0.50-BL-EP1.5
Class
D类功放
Speaker Channels
-
Output Power
3.2W×1@4Ω
Voltage - Supply
2.5V~5.5V
Total Harmonic Distortion + Noise (THD+N)
-
Quiescent Current
2.4mA
Operating Temperature
-40℃~+85℃
Power Supply Rejection Ratio (PSRR)
77dB
Efficiency
92%
Description
功放类型:D类功放;扬声器通道数:-;输出功率:3.2W×1@4Ω;静态电流(Iq):2.4mA;

*
]
[
DESIGNATOR
C7
FOOTPRINT
C0603
PARTTYPE
CC0603KRX7R9BB104
DESCRIPTION
容值:100nF;精度:±10%;额定电压:50V;温度系数:X7R;
Component Kind
Standard
Add into BOM
yes
Convert to PCB
yes
Symbol
CC0603KRX7R9BB104
Designator
C7
Device
CC0603KRX7R9BB104
Unique ID
gge24
Name
100nF
Reuse Block

Group ID

Channel ID

LCSC Part Name
100nF ±10% 50V
Supplier Part
C14663
Manufacturer
YAGEO(国巨)
Manufacturer Part
CC0603KRX7R9BB104
Supplier Footprint
0603
JLCPCB Part Class
Basic Part
Datasheet
https://item.szlcsc.com/datasheet/CC0603KRX7R9BB104/15331.html
Supplier
LCSC
3D Model Title
C0603_L1.6-W0.8-H0.8
Value
100nF
Tolerance
±10%
Voltage Rating
50V
Temperature Coefficient
X7R
Description
容值:100nF;精度:±10%;额定电压:50V;温度系数:X7R;

*
]
[
DESIGNATOR
C8
FOOTPRINT
C0603
PARTTYPE
CL10A106MA8NRNC
DESCRIPTION
容值:10uF;精度:±20%;额定电压:25V;温度系数:X5R;
Component Kind
Standard
Add into BOM
yes
Convert to PCB
yes
Symbol
CL10A106MA8NRNC
Designator
C8
Device
CL10A106MA8NRNC
Unique ID
gge25
Name
10uF
Reuse Block

Group ID

Channel ID

LCSC Part Name
10uF ±20% 25V
Supplier Part
C96446
Manufacturer
SAMSUNG(三星)
Manufacturer Part
CL10A106MA8NRNC
Supplier Footprint
0603
JLCPCB Part Class
Basic Part
Datasheet
https://item.szlcsc.com/datasheet/CL10A106MA8NRNC/97651.html
Supplier
LCSC
3D Model Title
C0603_L1.6-W0.8-H0.8
Value
10uF
Tolerance
±20%
Voltage Rating
25V
Temperature Coefficient
X5R
Description
容值:10uF;精度:±20%;额定电压:25V;温度系数:X5R;

*
]
[
DESIGNATOR
C10
FOOTPRINT
C0402
PARTTYPE
CL05B104KO5NNNC
DESCRIPTION
容值:100nF;精度:±10%;额定电压:16V;温度系数:X7R;
Component Kind
Standard
Add into BOM
yes
Convert to PCB
yes
Symbol
CL05B104KO5NNNC
Designator
C10
Device
CL05B104KO5NNNC
Unique ID
gge27
Name
100nF
Reuse Block

Group ID

Channel ID

LCSC Part Name
100nF ±10% 16V
Supplier Part
C1525
Manufacturer
SAMSUNG(三星)
Manufacturer Part
CL05B104KO5NNNC
Supplier Footprint
0402
JLCPCB Part Class
Basic Part
Datasheet
https://item.szlcsc.com/datasheet/CL05B104KO5NNNC/1877.html
Supplier
LCSC
3D Model Title
C0402_L1.0-W0.5-H0.5
Value
100nF
Tolerance
±10%
Voltage Rating
16V
Temperature Coefficient
X7R
Description
容值:100nF;精度:±10%;额定电压:16V;温度系数:X7R;

*
]
[
DESIGNATOR
C12
FOOTPRINT
C0402
PARTTYPE
CL05B104KO5NNNC
DESCRIPTION
容值:100nF;精度:±10%;额定电压:16V;温度系数:X7R;
Component Kind
Standard
Add into BOM
yes
Convert to PCB
yes
Symbol
CL05B104KO5NNNC
Designator
C12
Device
CL05B104KO5NNNC
Unique ID
gge28
Name
100nF
Reuse Block

Group ID

Channel ID

LCSC Part Name
100nF ±10% 16V
Supplier Part
C1525
Manufacturer
SAMSUNG(三星)
Manufacturer Part
CL05B104KO5NNNC
Supplier Footprint
0402
JLCPCB Part Class
Basic Part
Datasheet
https://item.szlcsc.com/datasheet/CL05B104KO5NNNC/1877.html
Supplier
LCSC
3D Model Title
C0402_L1.0-W0.5-H0.5
Value
100nF
Tolerance
±10%
Voltage Rating
16V
Temperature Coefficient
X7R
Description
容值:100nF;精度:±10%;额定电压:16V;温度系数:X7R;

*
]
[
DESIGNATOR
R7
FOOTPRINT
R0402
PARTTYPE
0402WGF5101TCE
DESCRIPTION
电阻类型:厚膜电阻;阻值:5.1kΩ;精度:±1%;功率:62.5mW;工作电压:50V;温度系数:±100ppm/℃;
Component Kind
Standard
Add into BOM
yes
Convert to PCB
yes
Symbol
0402WGF5101TCE
Designator
R7
Device
0402WGF5101TCE
Unique ID
gge29
Name
5.1kΩ
Reuse Block

Group ID

Channel ID

LCSC Part Name
5.1kΩ ±1% 62.5mW 厚膜电阻
Supplier Part
C25905
Manufacturer
UNI-ROYAL(厚声)
Manufacturer Part
0402WGF5101TCE
Supplier Footprint
0402
JLCPCB Part Class
Basic Part
Datasheet
https://item.szlcsc.com/datasheet/0402WGF5101TCE/26648.html
Supplier
LCSC
3D Model Title
R0402_L1.0-W0.5-H0.4
Type
厚膜电阻
Value
5.1kΩ
Tolerance
±1%
Power(Watts)
62.5mW
Voltage-Supply(Max)
50V
Temperature Coefficient
±100ppm/℃
Operating Temperature
-55℃~+155℃
Description
电阻类型:厚膜电阻;阻值:5.1kΩ;精度:±1%;功率:62.5mW;工作电压:50V;温度系数:±100ppm/℃;

*
]
[
DESIGNATOR
R6
FOOTPRINT
R0402
PARTTYPE
0402WGF5101TCE
DESCRIPTION
电阻类型:厚膜电阻;阻值:5.1kΩ;精度:±1%;功率:62.5mW;工作电压:50V;温度系数:±100ppm/℃;
Component Kind
Standard
Add into BOM
yes
Convert to PCB
yes
Symbol
0402WGF5101TCE
Designator
R6
Device
0402WGF5101TCE
Unique ID
gge30
Name
5.1kΩ
Reuse Block

Group ID

Channel ID

LCSC Part Name
5.1kΩ ±1% 62.5mW 厚膜电阻
Supplier Part
C25905
Manufacturer
UNI-ROYAL(厚声)
Manufacturer Part
0402WGF5101TCE
Supplier Footprint
0402
JLCPCB Part Class
Basic Part
Datasheet
https://item.szlcsc.com/datasheet/0402WGF5101TCE/26648.html
Supplier
LCSC
3D Model Title
R0402_L1.0-W0.5-H0.4
Type
厚膜电阻
Value
5.1kΩ
Tolerance
±1%
Power(Watts)
62.5mW
Voltage-Supply(Max)
50V
Temperature Coefficient
±100ppm/℃
Operating Temperature
-55℃~+155℃
Description
电阻类型:厚膜电阻;阻值:5.1kΩ;精度:±1%;功率:62.5mW;工作电压:50V;温度系数:±100ppm/℃;

*
]
[
DESIGNATOR
C13
FOOTPRINT
C0402
PARTTYPE
CL05B104KO5NNNC
DESCRIPTION
容值:100nF;精度:±10%;额定电压:16V;温度系数:X7R;
Component Kind
Standard
Add into BOM
yes
Convert to PCB
yes
Symbol
CL05B104KO5NNNC
Designator
C13
Device
CL05B104KO5NNNC
Name
100nF
Unique ID
gge31
Reuse Block

Group ID

Channel ID

LCSC Part Name
100nF ±10% 16V
Supplier Part
C1525
Manufacturer
SAMSUNG(三星)
Manufacturer Part
CL05B104KO5NNNC
Supplier Footprint
0402
JLCPCB Part Class
Basic Part
Datasheet
https://item.szlcsc.com/datasheet/CL05B104KO5NNNC/1877.html
Supplier
LCSC
3D Model Title
C0402_L1.0-W0.5-H0.5
Value
100nF
Tolerance
±10%
Voltage Rating
16V
Temperature Coefficient
X7R
Description
容值:100nF;精度:±10%;额定电压:16V;温度系数:X7R;

*
]
[
DESIGNATOR
J2
FOOTPRINT
CONN-TH_B8B-XH-AM-LF-SN
PARTTYPE
B8B-XH-AM(LF)(SN)
DESCRIPTION
插针结构:1x8P;间距:2.5mm;安装方式:直插;参考系列:XH;总PIN数:8P;排数:1;每排PIN数:8;行距:-;额定电流:3A;触头材质:黄铜;触头镀层:锡;工作温度:-25℃~+85℃;
Component Kind
Standard
Add into BOM
yes
Convert to PCB
yes
Symbol
B8B-XH-AM (LF)(SN)
Designator
J2
Device
B8B-XH-AM(LF)(SN)
Unique ID
gge33
Name
B8B-XH-AM(LF)(SN)
Reuse Block

Group ID

Channel ID

LCSC Part Name
1x8P 间距:2.5mm 直插 系列:XH
Supplier Part
C161875
Manufacturer
JST
Manufacturer Part
B8B-XH-AM(LF)(SN)
Supplier Footprint
插件,P=2.5mm
JLCPCB Part Class
Extended Part
Datasheet
https://item.szlcsc.com/datasheet/B8B-XH-AM(LF)(SN)/173256.html
Supplier
LCSC
3D Model Title
CONN-TH_B8B-XH-AM (LF)(SN)
Pins Structure
1x8P
Pitch
2.5mm
Mounting Type
直插
Reference Series
XH
Number of Pins
8P
Number of Rows
1
Number of PINs Per Row
8
Row Spacing
-
Current Rating
3A
Contact Material
黄铜
Contact Plating
锡
Operating Temperature
-25℃~+85℃
Voltage Rating
250V
Plastic Material
PA66
Flame Retardant Rating
UL94V-0
Supplementary Features
带柱；打K脚
Color
白色
Z-Height of the Board
7mm
X-Length of Bottom Edge on Board (Spacing Line)
22.4mm
Y-Width of Bottom Edge on Board
5.75mm
Description
插针结构:1x8P;间距:2.5mm;安装方式:直插;参考系列:XH;总PIN数:8P;排数:1;每排PIN数:8;行距:-;额定电流:3A;触头材质:黄铜;触头镀层:锡;工作温度:-25℃~+85℃;

*
]
[
DESIGNATOR
D1
FOOTPRINT
LED-SMD_L1.6-W0.8-R-RD
PARTTYPE
KT-0603R
DESCRIPTION
灯头类型:1.6mmx0.8mm方形灯头;发光颜色:红色;正向压降(Vf):1.8V~2.4V;功率:40mW;正向电流:20mA;波长:615nm~630nm;二极管配置:独立二极管;透镜颜色:无色透明透镜;色温:-;发光强度:300mcd;发光角度:120°;载带方式:-;工作温度:-40℃~+85℃;
Component Kind
Standard
Add into BOM
yes
Convert to PCB
yes
Symbol
KT-0603R
Designator
D1
Device
KT-0603R
Name
KT-0603R
Unique ID
gge15_0
Reuse Block

Group ID

Channel ID

LCSC Part Name
0603 红灯 高亮
Supplier Part
C2286
Manufacturer
KENTO
Manufacturer Part
KT-0603R
Supplier Footprint
0603
JLCPCB Part Class
Basic Part
Datasheet
https://item.szlcsc.com/datasheet/KT-0603R/2659.html
Supplier
LCSC
3D Model Title
LED0603_L1.6-W0.8-H0.6
Lamp Holder Type
1.6mmx0.8mm方形灯头
Illumination Color
红色
Voltage - Forward(Vf)
1.8V~2.4V
Power(Watts)
40mW
Forward Current
20mA
Wavelength - Dominant
615nm~630nm
Peak Wavelength
645nm
Diode Configuration
独立二极管
Lens Color
无色透明透镜
Color Temperature
-
Luminous Intensity
300mcd
Viewing Angle
120°
Mounting Style
-
Operating Temperature
-40℃~+85℃
Description
灯头类型:1.6mmx0.8mm方形灯头;发光颜色:红色;正向压降(Vf):1.8V~2.4V;功率:40mW;正向电流:20mA;波长:615nm~630nm;二极管配置:独立二极管;透镜颜色:无色透明透镜;色温:-;发光强度:300mcd;发光角度:120°;载带方式:-;工作温度:-40℃~+85℃;

*
]
[
DESIGNATOR
J1
FOOTPRINT
USB-C-SMD_TYPE-C-16PIN-2MD-073
PARTTYPE
TYPE-C 16PIN 2MD(073)
DESCRIPTION
连接器类型:Type-C;协议标准:-;公母:母;安装方式:卧贴;触点数量:16P;端口数量:1;额定电流 - 电源:3A;工作温度:-25℃~+85℃;
Component Kind
Standard
Add into BOM
yes
Convert to PCB
yes
Symbol
TYPE-C 16PIN 2MD(073)
Designator
J1
Device
TYPE-C 16PIN 2MD(073)
Unique ID
gge37
Name
TYPE-C 16PIN 2MD(073)
Reuse Block

Group ID

Channel ID

LCSC Part Name
Type-C 母 卧贴
Supplier Part
C2765186
Manufacturer
SHOU HAN(首韩)
Manufacturer Part
TYPE-C 16PIN 2MD(073)
Supplier Footprint
SMD
JLCPCB Part Class
Extended Part
Datasheet
https://item.szlcsc.com/datasheet/TYPE-C%252016PIN%25202MD(073)/2901843.html
Supplier
LCSC
3D Model Title
USB-C-SMD_TYPE-C-6PIN-2MD-073
Connector Type
Type-C
Protocol Standard
-
Gender
母
Mounting Type
卧贴
Number of Contacts
16P
Number of Ports
1
Current Rating-Power
3A
Voltage Rating
5V
Connect-Disconnect Life
1万次
Supplementary Features
-
Center Height
-
Length
-
Detection color
黑色
Operating Temperature
-25℃~+85℃
Description
连接器类型:Type-C;协议标准:-;公母:母;安装方式:卧贴;触点数量:16P;端口数量:1;额定电流 - 电源:3A;工作温度:-25℃~+85℃;

*
]
[
DESIGNATOR
C9
FOOTPRINT
C0603
PARTTYPE
CL10A106MA8NRNC
DESCRIPTION
容值:10uF;精度:±20%;额定电压:25V;温度系数:X5R;
Component Kind
Standard
Add into BOM
yes
Convert to PCB
yes
Symbol
CL10A106MA8NRNC
Designator
C9
Device
CL10A106MA8NRNC
Unique ID
gge41
LCSC Part Name
10uF ±20% 25V
Supplier Part
C96446
Manufacturer
SAMSUNG(三星)
Manufacturer Part
CL10A106MA8NRNC
Supplier Footprint
0603
JLCPCB Part Class
Basic Part
Datasheet
https://item.szlcsc.com/datasheet/CL10A106MA8NRNC/97651.html
Supplier
LCSC
3D Model Title
C0603_L1.6-W0.8-H0.8
Value
10uF
Tolerance
±20%
Voltage Rating
25V
Temperature Coefficient
X5R
Name
10uF
Description
容值:10uF;精度:±20%;额定电压:25V;温度系数:X5R;
Reuse Block

Group ID

Channel ID


*
]
[
DESIGNATOR
C14
FOOTPRINT
C0603
PARTTYPE
CC0603KRX7R9BB104
DESCRIPTION
容值:100nF;精度:±10%;额定电压:50V;温度系数:X7R;
Component Kind
Standard
Add into BOM
yes
Convert to PCB
yes
Symbol
CC0603KRX7R9BB104
Designator
C14
Device
CC0603KRX7R9BB104
Unique ID
gge42
LCSC Part Name
100nF ±10% 50V
Supplier Part
C14663
Manufacturer
YAGEO(国巨)
Manufacturer Part
CC0603KRX7R9BB104
Supplier Footprint
0603
JLCPCB Part Class
Basic Part
Datasheet
https://item.szlcsc.com/datasheet/CC0603KRX7R9BB104/15331.html
Supplier
LCSC
3D Model Title
C0603_L1.6-W0.8-H0.8
Value
100nF
Tolerance
±10%
Voltage Rating
50V
Temperature Coefficient
X7R
Name
100nF
Description
容值:100nF;精度:±10%;额定电压:50V;温度系数:X7R;
Reuse Block

Group ID

Channel ID


*
]
[
DESIGNATOR
C11
FOOTPRINT
C0603
PARTTYPE
CL10A106MA8NRNC
DESCRIPTION
容值:10uF;精度:±20%;额定电压:25V;温度系数:X5R;
Component Kind
Standard
Add into BOM
yes
Convert to PCB
yes
Symbol
CL10A106MA8NRNC
Designator
C11
Device
CL10A106MA8NRNC
Unique ID
gge41_1
LCSC Part Name
10uF ±20% 25V
Supplier Part
C96446
Manufacturer
SAMSUNG(三星)
Manufacturer Part
CL10A106MA8NRNC
Supplier Footprint
0603
JLCPCB Part Class
Basic Part
Datasheet
https://item.szlcsc.com/datasheet/CL10A106MA8NRNC/97651.html
Supplier
LCSC
3D Model Title
C0603_L1.6-W0.8-H0.8
Value
10uF
Tolerance
±20%
Voltage Rating
25V
Temperature Coefficient
X5R
Name
10uF
Description
容值:10uF;精度:±20%;额定电压:25V;温度系数:X5R;
Reuse Block

Group ID

Channel ID


*
]
[
DESIGNATOR
C5
FOOTPRINT
C0603
PARTTYPE
CL10A225KO8NNNC
DESCRIPTION
容值:2.2uF;精度:±10%;额定电压:16V;温度系数:X5R;
Component Kind
Standard
Add into BOM
yes
Convert to PCB
yes
Symbol
CL10A225KO8NNNC
Designator
C5
Device
CL10A225KO8NNNC
Unique ID
gge44
Name
2.2uF
Reuse Block

Group ID

Channel ID

LCSC Part Name
2.2uF ±10% 16V
Supplier Part
C23630
Manufacturer
SAMSUNG(三星)
Manufacturer Part
CL10A225KO8NNNC
Supplier Footprint
0603
JLCPCB Part Class
Basic Part
Datasheet
https://item.szlcsc.com/datasheet/CL10A225KO8NNNC/24366.html
Supplier
LCSC
3D Model Title
C0603_L1.6-W0.8-H0.8
Value
2.2uF
Tolerance
±10%
Voltage Rating
16V
Temperature Coefficient
X5R
Description
容值:2.2uF;精度:±10%;额定电压:16V;温度系数:X5R;

*
]
[
DESIGNATOR
C6
FOOTPRINT
C0603
PARTTYPE
CL10A225KO8NNNC
DESCRIPTION
容值:2.2uF;精度:±10%;额定电压:16V;温度系数:X5R;
Component Kind
Standard
Add into BOM
yes
Convert to PCB
yes
Symbol
CL10A225KO8NNNC
Designator
C6
Device
CL10A225KO8NNNC
Name
2.2uF
Unique ID
gge45
Reuse Block

Group ID

Channel ID

LCSC Part Name
2.2uF ±10% 16V
Supplier Part
C23630
Manufacturer
SAMSUNG(三星)
Manufacturer Part
CL10A225KO8NNNC
Supplier Footprint
0603
JLCPCB Part Class
Basic Part
Datasheet
https://item.szlcsc.com/datasheet/CL10A225KO8NNNC/24366.html
Supplier
LCSC
3D Model Title
C0603_L1.6-W0.8-H0.8
Value
2.2uF
Tolerance
±10%
Voltage Rating
16V
Temperature Coefficient
X5R
Description
容值:2.2uF;精度:±10%;额定电压:16V;温度系数:X5R;

*
]
[
DESIGNATOR
J4
FOOTPRINT
CONN-TH_3P-P2.50_A2501WV2-3P
PARTTYPE
B3B-XH-A(LF)(SN)
DESCRIPTION
插针结构:1x3P;间距:2.5mm;安装方式:直插;参考系列:XH;总PIN数:3P;排数:1;每排PIN数:3;行距:-;额定电流:3A;触头材质:黄铜;触头镀层:锡;工作温度:-25℃~+85℃;
Component Kind
Standard
Add into BOM
yes
Convert to PCB
yes
Symbol
B3B-XH-A(LF)(SN)
Designator
J4
Device
B3B-XH-A(LF)(SN)
Unique ID
gge46
Name
B3B-XH-A(LF)(SN)
Reuse Block

Group ID

Channel ID

LCSC Part Name
1x3P 间距:2.5mm 直插 系列:XH
Supplier Part
C144394
Manufacturer
JST
Manufacturer Part
B3B-XH-A(LF)(SN)
Supplier Footprint
插件,P=2.5mm
JLCPCB Part Class
Extended Part
Datasheet
https://item.szlcsc.com/datasheet/B3B-XH-A(LF)(SN)/155726.html
Supplier
LCSC
3D Model Title
CONN-TH_3P-P2.50_A2501WV2-3P
Pins Structure
1x3P
Pitch
2.5mm
Mounting Type
直插
Reference Series
XH
Number of Pins
3P
Number of Rows
1
Number of PINs Per Row
3
Row Spacing
-
Current Rating
3A
Contact Material
黄铜
Contact Plating
锡
Operating Temperature
-25℃~+85℃
Voltage Rating
250V
Plastic Material
PA66
Flame Retardant Rating
UL94V-0
Supplementary Features
打K脚
Color
白色
Z-Height of the Board
7mm
X-Length of Bottom Edge on Board (Spacing Line)
9.9mm
Y-Width of Bottom Edge on Board
5.75mm
Description
插针结构:1x3P;间距:2.5mm;安装方式:直插;参考系列:XH;总PIN数:3P;排数:1;每排PIN数:3;行距:-;额定电流:3A;触头材质:黄铜;触头镀层:锡;工作温度:-25℃~+85℃;

*
]
[
DESIGNATOR
U1
FOOTPRINT
QFN-56_L7.0-W7.0-P0.40-BL-EP5.7
PARTTYPE
ESP32-S3FH4R2
DESCRIPTION
核心芯片:LX7芯片;频率:2.4GHz;天线形式:-;发射功率:21dBm;接收灵敏度:-104.5dBm;
Component Kind
Standard
Add into BOM
yes
Convert to PCB
yes
Symbol
ESP32-S3FH4R2
Designator
U1
Device
ESP32-S3FH4R2
Unique ID
gge90
Name
2.4GHz
Reuse Block

Group ID

Channel ID

LCSC Part Name
不带固件 Xtensa 32位Lx7双核微处理器，2.4 GHz Wi-Fi和Bluetooth 5(LE)，45个GPIO管脚
Supplier Part
C3013940
Manufacturer
ESPRESSIF(乐鑫)
Manufacturer Part
ESP32-S3FH4R2
Supplier Footprint
QFN-56(7x7)
JLCPCB Part Class
Extended Part
Datasheet
https://item.szlcsc.com/datasheet/ESP32-S3FH4R2/3522410.html
Supplier
LCSC
Utilized IC / Part
LX7芯片
Wireless Standard
Bluetooth5.0
Interface Type
SDIO；JTAG；UART；SPI；I2C
Value
2.4GHz
Antenna Type
-
Output Power
21dBm
Voltage - Supply
3V~3.6V
Receive  Current
88mA
Send  Current
340mA
Sensitivity
-104.5dBm
Operating Temperature
-40℃~+85℃
Description
核心芯片:LX7芯片;频率:2.4GHz;天线形式:-;发射功率:21dBm;接收灵敏度:-104.5dBm;

*
]
[
DESIGNATOR
R1
FOOTPRINT
R0402
PARTTYPE
0402WGF1002TCE
DESCRIPTION
电阻类型:厚膜电阻;阻值:10kΩ;精度:±1%;功率:62.5mW;工作电压:50V;温度系数:±100ppm/℃;
Component Kind
Standard
Add into BOM
yes
Convert to PCB
yes
Symbol
0402WGF1002TCE
Designator
R1
Device
0402WGF1002TCE
Unique ID
gge12
Name
10kΩ
Reuse Block

Group ID

Channel ID

LCSC Part Name
10kΩ ±1% 62.5mW 厚膜电阻
Supplier Part
C25744
Manufacturer
UNI-ROYAL(厚声)
Manufacturer Part
0402WGF1002TCE
Supplier Footprint
0402
JLCPCB Part Class
Basic Part
Datasheet
https://item.szlcsc.com/datasheet/0402WGF1002TCE/26487.html
Supplier
LCSC
3D Model Title
R0402_L1.0-W0.5-H0.4
Type
厚膜电阻
Value
10kΩ
Tolerance
±1%
Power(Watts)
62.5mW
Voltage-Supply(Max)
50V
Temperature Coefficient
±100ppm/℃
Operating Temperature
-55℃~+155℃
Description
电阻类型:厚膜电阻;阻值:10kΩ;精度:±1%;功率:62.5mW;工作电压:50V;温度系数:±100ppm/℃;

*
]
[
DESIGNATOR
BOOT
FOOTPRINT
SW-SMD_L3.9-W3.0-P4.45
PARTTYPE
TS-1088-AR02016
DESCRIPTION
电路结构:单刀单掷;按钮形状:圆形按钮;作用力:1.6N;安装方式:立贴;开关长度:3.9mm;开关宽度:3mm;开关高度:2mm;带支架:不带支架;触点电流:50mA;额定电压:12V;带灯:-;工作寿命:10万次;
Component Kind
Standard
Add into BOM
yes
Convert to PCB
yes
Symbol
TS-1088-AR02016
Designator
BOOT
Device
TS-1088-AR02016
Unique ID
gge13
Name
TS-1088-AR02016
Reuse Block

Group ID

Channel ID

LCSC Part Name
3.9*3*2mm 立贴 轻触开关
Supplier Part
C720477
Manufacturer
XUNPU(讯普)
Manufacturer Part
TS-1088-AR02016
Supplier Footprint
SMD,4x3mm
JLCPCB Part Class
Basic Part
Datasheet
https://item.szlcsc.com/datasheet/TS-1088-AR02016/763484.html
Supplier
LCSC
3D Model Title
SW-SMD_L3.9-W2.9-H2.0-LS4.8
Circuit
单刀单掷
Actuator Style
圆形按钮
Operating Force
1.6N
Mounting Type
立贴
Length
3.9mm
Width
3mm
Switch Height
2mm
with Bracket
不带支架
Contact Current
50mA
Voltage Rating
12V
Actuator/Cap Color
黑色
With Lamp
-
IP Rating
-
Termination Style
SMD接片
Life
10万次
Operating Temperature
-30℃~+80℃
Description
电路结构:单刀单掷;按钮形状:圆形按钮;作用力:1.6N;安装方式:立贴;开关长度:3.9mm;开关宽度:3mm;开关高度:2mm;带支架:不带支架;触点电流:50mA;额定电压:12V;带灯:-;工作寿命:10万次;

*
]
[
DESIGNATOR
R3
FOOTPRINT
R0402
PARTTYPE
0402WGF4701TCE
DESCRIPTION
电阻类型:厚膜电阻;阻值:4.7kΩ;精度:±1%;功率:62.5mW;工作电压:50V;温度系数:±100ppm/℃;
Component Kind
Standard
Add into BOM
yes
Convert to PCB
yes
Symbol
0402WGF4701TCE
Designator
R3
Device
0402WGF4701TCE
Unique ID
gge16
Name
4.7kΩ
Reuse Block

Group ID

Channel ID

LCSC Part Name
4.7kΩ ±1% 62.5mW 厚膜电阻
Supplier Part
C25900
Manufacturer
UNI-ROYAL(厚声)
Manufacturer Part
0402WGF4701TCE
Supplier Footprint
0402
JLCPCB Part Class
Basic Part
Datasheet
https://item.szlcsc.com/datasheet/0402WGF4701TCE/26643.html
Supplier
LCSC
3D Model Title
R0402_L1.0-W0.5-H0.4
Type
厚膜电阻
Value
4.7kΩ
Tolerance
±1%
Power(Watts)
62.5mW
Voltage-Supply(Max)
50V
Temperature Coefficient
±100ppm/℃
Operating Temperature
-55℃~+155℃
Description
电阻类型:厚膜电阻;阻值:4.7kΩ;精度:±1%;功率:62.5mW;工作电压:50V;温度系数:±100ppm/℃;

*
]
[
DESIGNATOR
R4
FOOTPRINT
R0402
PARTTYPE
0402WGF4701TCE
DESCRIPTION
电阻类型:厚膜电阻;阻值:4.7kΩ;精度:±1%;功率:62.5mW;工作电压:50V;温度系数:±100ppm/℃;
Component Kind
Standard
Add into BOM
yes
Convert to PCB
yes
Symbol
0402WGF4701TCE
Designator
R4
Device
0402WGF4701TCE
Unique ID
gge17
Name
4.7kΩ
Reuse Block

Group ID

Channel ID

LCSC Part Name
4.7kΩ ±1% 62.5mW 厚膜电阻
Supplier Part
C25900
Manufacturer
UNI-ROYAL(厚声)
Manufacturer Part
0402WGF4701TCE
Supplier Footprint
0402
JLCPCB Part Class
Basic Part
Datasheet
https://item.szlcsc.com/datasheet/0402WGF4701TCE/26643.html
Supplier
LCSC
3D Model Title
R0402_L1.0-W0.5-H0.4
Type
厚膜电阻
Value
4.7kΩ
Tolerance
±1%
Power(Watts)
62.5mW
Voltage-Supply(Max)
50V
Temperature Coefficient
±100ppm/℃
Operating Temperature
-55℃~+155℃
Description
电阻类型:厚膜电阻;阻值:4.7kΩ;精度:±1%;功率:62.5mW;工作电压:50V;温度系数:±100ppm/℃;

*
]
[
DESIGNATOR
R9
FOOTPRINT
R0402
PARTTYPE
0402WGF220JTCE
DESCRIPTION
电阻类型:厚膜电阻;阻值:22Ω;精度:±1%;功率:62.5mW;最大工作电压:50V;温度系数:±100ppm/℃;
Component Kind
Standard
Add into BOM
yes
Convert to PCB
yes
Symbol
0402WGF220JTCE
Designator
R9
Device
0402WGF220JTCE
Unique ID
gge39
Name
22Ω
Reuse Block

Group ID

Channel ID

LCSC Part Name
22Ω ±1% 62.5mW 厚膜电阻
Supplier Part
C25092
Manufacturer
UNI-ROYAL(厚声)
Manufacturer Part
0402WGF220JTCE
Supplier Footprint
0402
JLCPCB Part Class
Basic Part
Datasheet
https://atta.szlcsc.com/upload/public/pdf/source/20200306/C422600_1E6D84923E4A46A82E41ADD87F860B5C.pdf
Supplier
LCSC
3D Model Title
R0402_L1.0-W0.5-H0.4
Type
厚膜电阻
Value
22Ω
Tolerance
±1%
Power(Watts)
62.5mW
Overload Voltage (Max)
50V
Temperature Coefficient
±100ppm/℃
Operating Temperature Range
-55℃~+155℃
Description
电阻类型:厚膜电阻;阻值:22Ω;精度:±1%;功率:62.5mW;最大工作电压:50V;温度系数:±100ppm/℃;

*
]
[
DESIGNATOR
R10
FOOTPRINT
R0402
PARTTYPE
0402WGF220JTCE
DESCRIPTION
电阻类型:厚膜电阻;阻值:22Ω;精度:±1%;功率:62.5mW;最大工作电压:50V;温度系数:±100ppm/℃;
Component Kind
Standard
Add into BOM
yes
Convert to PCB
yes
Symbol
0402WGF220JTCE
Designator
R10
Device
0402WGF220JTCE
Unique ID
gge40
Name
22Ω
Reuse Block

Group ID

Channel ID

LCSC Part Name
22Ω ±1% 62.5mW 厚膜电阻
Supplier Part
C25092
Manufacturer
UNI-ROYAL(厚声)
Manufacturer Part
0402WGF220JTCE
Supplier Footprint
0402
JLCPCB Part Class
Basic Part
Datasheet
https://atta.szlcsc.com/upload/public/pdf/source/20200306/C422600_1E6D84923E4A46A82E41ADD87F860B5C.pdf
Supplier
LCSC
3D Model Title
R0402_L1.0-W0.5-H0.4
Type
厚膜电阻
Value
22Ω
Tolerance
±1%
Power(Watts)
62.5mW
Overload Voltage (Max)
50V
Temperature Coefficient
±100ppm/℃
Operating Temperature Range
-55℃~+155℃
Description
电阻类型:厚膜电阻;阻值:22Ω;精度:±1%;功率:62.5mW;最大工作电压:50V;温度系数:±100ppm/℃;

*
]
[
DESIGNATOR
R5
FOOTPRINT
R0402
PARTTYPE
0402WGF1002TCE
DESCRIPTION
电阻类型:厚膜电阻;阻值:10kΩ;精度:±1%;功率:62.5mW;工作电压:50V;温度系数:±100ppm/℃;
Component Kind
Standard
Add into BOM
yes
Convert to PCB
yes
Symbol
0402WGF1002TCE
Designator
R5
Device
0402WGF1002TCE
Name
10kΩ
Unique ID
gge18
Reuse Block

Group ID

Channel ID

LCSC Part Name
10kΩ ±1% 62.5mW 厚膜电阻
Supplier Part
C25744
Manufacturer
UNI-ROYAL(厚声)
Manufacturer Part
0402WGF1002TCE
Supplier Footprint
0402
JLCPCB Part Class
Basic Part
Datasheet
https://item.szlcsc.com/datasheet/0402WGF1002TCE/26487.html
Supplier
LCSC
3D Model Title
R0402_L1.0-W0.5-H0.4
Type
厚膜电阻
Value
10kΩ
Tolerance
±1%
Power(Watts)
62.5mW
Voltage-Supply(Max)
50V
Temperature Coefficient
±100ppm/℃
Operating Temperature
-55℃~+155℃
Description
电阻类型:厚膜电阻;阻值:10kΩ;精度:±1%;功率:62.5mW;工作电压:50V;温度系数:±100ppm/℃;

*
]
[
DESIGNATOR
RESET
FOOTPRINT
SW-SMD_L3.9-W3.0-P4.45
PARTTYPE
TS-1088-AR02016
DESCRIPTION
电路结构:单刀单掷;按钮形状:圆形按钮;作用力:1.6N;安装方式:立贴;开关长度:3.9mm;开关宽度:3mm;开关高度:2mm;带支架:不带支架;触点电流:50mA;额定电压:12V;带灯:-;工作寿命:10万次;
Component Kind
Standard
Add into BOM
yes
Convert to PCB
yes
Symbol
TS-1088-AR02016
Designator
RESET
Device
TS-1088-AR02016
Name
TS-1088-AR02016
Unique ID
gge19
Reuse Block

Group ID

Channel ID

LCSC Part Name
3.9*3*2mm 立贴 轻触开关
Supplier Part
C720477
Manufacturer
XUNPU(讯普)
Manufacturer Part
TS-1088-AR02016
Supplier Footprint
SMD,4x3mm
JLCPCB Part Class
Basic Part
Datasheet
https://item.szlcsc.com/datasheet/TS-1088-AR02016/763484.html
Supplier
LCSC
3D Model Title
SW-SMD_L3.9-W2.9-H2.0-LS4.8
Circuit
单刀单掷
Actuator Style
圆形按钮
Operating Force
1.6N
Mounting Type
立贴
Length
3.9mm
Width
3mm
Switch Height
2mm
with Bracket
不带支架
Contact Current
50mA
Voltage Rating
12V
Actuator/Cap Color
黑色
With Lamp
-
IP Rating
-
Termination Style
SMD接片
Life
10万次
Operating Temperature
-30℃~+80℃
Description
电路结构:单刀单掷;按钮形状:圆形按钮;作用力:1.6N;安装方式:立贴;开关长度:3.9mm;开关宽度:3mm;开关高度:2mm;带支架:不带支架;触点电流:50mA;额定电压:12V;带灯:-;工作寿命:10万次;

*
]
[
DESIGNATOR
C4
FOOTPRINT
C0402
PARTTYPE
CL05A105KA5NQNC
DESCRIPTION
容值:1uF;精度:±10%;额定电压:25V;温度系数:X5R;
Component Kind
Standard
Add into BOM
yes
Convert to PCB
yes
Symbol
CL05A105KA5NQNC
Designator
C4
Device
CL05A105KA5NQNC
Name
1uF
Unique ID
gge20
Reuse Block

Group ID

Channel ID

LCSC Part Name
1uF ±10% 25V
Supplier Part
C52923
Manufacturer
SAMSUNG(三星)
Manufacturer Part
CL05A105KA5NQNC
Supplier Footprint
0402
JLCPCB Part Class
Basic Part
Datasheet
https://item.szlcsc.com/datasheet/CL05A105KA5NQNC/53938.html
Supplier
LCSC
3D Model Title
C0402_L1.0-W0.5-H0.5
Value
1uF
Tolerance
±10%
Voltage Rating
25V
Temperature Coefficient
X5R
Description
容值:1uF;精度:±10%;额定电压:25V;温度系数:X5R;

*
]
[
DESIGNATOR
R11
FOOTPRINT
R0402
PARTTYPE
0402WGF1002TCE
DESCRIPTION
电阻类型:厚膜电阻;阻值:10kΩ;精度:±1%;功率:62.5mW;工作电压:50V;温度系数:±100ppm/℃;
Component Kind
Standard
Add into BOM
yes
Convert to PCB
yes
Symbol
0402WGF1002TCE
Designator
R11
Device
0402WGF1002TCE
Unique ID
gge12_0
Name
10kΩ
Reuse Block

Group ID

Channel ID

LCSC Part Name
10kΩ ±1% 62.5mW 厚膜电阻
Supplier Part
C25744
Manufacturer
UNI-ROYAL(厚声)
Manufacturer Part
0402WGF1002TCE
Supplier Footprint
0402
JLCPCB Part Class
Basic Part
Datasheet
https://item.szlcsc.com/datasheet/0402WGF1002TCE/26487.html
Supplier
LCSC
3D Model Title
R0402_L1.0-W0.5-H0.4
Type
厚膜电阻
Value
10kΩ
Tolerance
±1%
Power(Watts)
62.5mW
Voltage-Supply(Max)
50V
Temperature Coefficient
±100ppm/℃
Operating Temperature
-55℃~+155℃
Description
电阻类型:厚膜电阻;阻值:10kΩ;精度:±1%;功率:62.5mW;工作电压:50V;温度系数:±100ppm/℃;

*
]
[
DESIGNATOR
R12
FOOTPRINT
R0402
PARTTYPE
0402WGF1002TCE
DESCRIPTION
电阻类型:厚膜电阻;阻值:10kΩ;精度:±1%;功率:62.5mW;工作电压:50V;温度系数:±100ppm/℃;
Component Kind
Standard
Add into BOM
yes
Convert to PCB
yes
Symbol
0402WGF1002TCE
Designator
R12
Device
0402WGF1002TCE
Unique ID
gge12_1
Name
10kΩ
Reuse Block

Group ID

Channel ID

LCSC Part Name
10kΩ ±1% 62.5mW 厚膜电阻
Supplier Part
C25744
Manufacturer
UNI-ROYAL(厚声)
Manufacturer Part
0402WGF1002TCE
Supplier Footprint
0402
JLCPCB Part Class
Basic Part
Datasheet
https://item.szlcsc.com/datasheet/0402WGF1002TCE/26487.html
Supplier
LCSC
3D Model Title
R0402_L1.0-W0.5-H0.4
Type
厚膜电阻
Value
10kΩ
Tolerance
±1%
Power(Watts)
62.5mW
Voltage-Supply(Max)
50V
Temperature Coefficient
±100ppm/℃
Operating Temperature
-55℃~+155℃
Description
电阻类型:厚膜电阻;阻值:10kΩ;精度:±1%;功率:62.5mW;工作电压:50V;温度系数:±100ppm/℃;

*
]
[
DESIGNATOR
L1
FOOTPRINT
L0402
PARTTYPE
LQW15AN24NG00D
DESCRIPTION
电感值:24nH;精度:±2%;额定电流:280mA;饱和电流(Isat):-;类型:非屏蔽电感;
Component Kind
Standard
Add into BOM
yes
Convert to PCB
yes
Symbol
LQW15AN24NG00D
Designator
L1
Device
LQW15AN24NG00D
Unique ID
gge59
Name
24nH
Reuse Block

Group ID

Channel ID

LCSC Part Name
24nH ±2%
Supplier Part
C167472
Manufacturer
muRata(村田)
Manufacturer Part
LQW15AN24NG00D
Supplier Footprint
0402
JLCPCB Part Class
Extended Part
Datasheet
https://item.szlcsc.com/datasheet/LQW15AN24NG00D/178855.html
Supplier
LCSC
3D Model Title
L0402_L1.0-W0.5-H0.5_BEAD
Value
24nH
Tolerance
±2%
Current Rating
280mA
Current - Saturation(Isat)
-
DC Resistance(DCR)
520mΩ
Type
非屏蔽电感
Ratings
-
Description
电感值:24nH;精度:±2%;额定电流:280mA;饱和电流(Isat):-;类型:非屏蔽电感;

*
]
[
DESIGNATOR
C16
FOOTPRINT
C0402
PARTTYPE
0402CG220J500NT
DESCRIPTION
容值:22pF;精度:±5%;额定电压:50V;温度系数:C0G;
Component Kind
Standard
Add into BOM
yes
Convert to PCB
yes
Symbol
0402CG220J500NT
Designator
C16
Device
0402CG220J500NT
Unique ID
gge60
Name
22pF
Reuse Block

Group ID

Channel ID

LCSC Part Name
22pF ±5% 50V
Supplier Part
C1555
Manufacturer
FH(风华)
Manufacturer Part
0402CG220J500NT
Supplier Footprint
0402
JLCPCB Part Class
Basic Part
Datasheet
https://item.szlcsc.com/datasheet/0402CG220J500NT/1907.html
Supplier
LCSC
3D Model Title
C0402_L1.0-W0.5-H0.5
Value
22pF
Tolerance
±5%
Voltage Rating
50V
Temperature Coefficient
C0G
Description
容值:22pF;精度:±5%;额定电压:50V;温度系数:C0G;

*
]
[
DESIGNATOR
C17
FOOTPRINT
C0402
PARTTYPE
0402CG220J500NT
DESCRIPTION
容值:22pF;精度:±5%;额定电压:50V;温度系数:C0G;
Component Kind
Standard
Add into BOM
yes
Convert to PCB
yes
Symbol
0402CG220J500NT
Designator
C17
Device
0402CG220J500NT
Unique ID
gge61
Name
22pF
Reuse Block

Group ID

Channel ID

LCSC Part Name
22pF ±5% 50V
Supplier Part
C1555
Manufacturer
FH(风华)
Manufacturer Part
0402CG220J500NT
Supplier Footprint
0402
JLCPCB Part Class
Basic Part
Datasheet
https://item.szlcsc.com/datasheet/0402CG220J500NT/1907.html
Supplier
LCSC
3D Model Title
C0402_L1.0-W0.5-H0.5
Value
22pF
Tolerance
±5%
Voltage Rating
50V
Temperature Coefficient
C0G
Description
容值:22pF;精度:±5%;额定电压:50V;温度系数:C0G;

*
]
[
DESIGNATOR
X1
FOOTPRINT
CRYSTAL-SMD_4P-L2.5-W2.0-BL
PARTTYPE
TXM40M0004252HBCEO00T
DESCRIPTION
晶振类型:贴片晶振;频率:40MHz;常温频差:±10ppm;负载电容:15pF;频率稳定度:±30ppm;
Component Kind
Standard
Add into BOM
yes
Convert to PCB
yes
Symbol
TXM40M0004252HBCEO00T
Designator
X1
Device
TXM40M0004252HBCEO00T
Unique ID
gge91
Name
40MHz
Reuse Block

Group ID

Channel ID

LCSC Part Name
40MHz ±10ppm 15pF
Supplier Part
C284176
Manufacturer
YJX(雅晶鑫)
Manufacturer Part
TXM40M0004252HBCEO00T
Supplier Footprint
SMD2520-4P
JLCPCB Part Class
Extended Part
Datasheet
https://item.szlcsc.com/datasheet/TXM40M0004252HBCEO00T/270225.html
Supplier
LCSC
3D Model Title
CRYSTAL-SMD_4P-L2.5-W2.0-BL
Type
贴片晶振
Value
40MHz
Normal temperature Frequency Tolerance
±10ppm
Load Capacitance
15pF
Frequency Stability
±30ppm
Equivalent Series Resistance(ESR)
25Ω
Operating Temperature
-40℃~+85℃
Description
晶振类型:贴片晶振;频率:40MHz;常温频差:±10ppm;负载电容:15pF;频率稳定度:±30ppm;

*
]
[
DESIGNATOR
C1
FOOTPRINT
C0402
PARTTYPE
CL05B104KB54PNC
DESCRIPTION
容值:100nF;精度:±10%;额定电压:50V;温度系数:X7R;
Component Kind
Standard
Add into BOM
yes
Convert to PCB
yes
Symbol
CL05B104KB54PNC
Designator
C1
Device
CL05B104KB54PNC
Unique ID
gge9
Name
100nF
Reuse Block

Group ID

Channel ID

LCSC Part Name
100nF ±10% 50V
Supplier Part
C307331
Manufacturer
SAMSUNG(三星)
Manufacturer Part
CL05B104KB54PNC
Supplier Footprint
0402
JLCPCB Part Class
Basic Part
Datasheet
https://item.szlcsc.com/datasheet/CL05B104KB54PNC/291005.html
Supplier
LCSC
3D Model Title
C0402_L1.0-W0.5-H0.5
Value
100nF
Tolerance
±10%
Voltage Rating
50V
Temperature Coefficient
X7R
Description
容值:100nF;精度:±10%;额定电压:50V;温度系数:X7R;

*
]
[
DESIGNATOR
C15
FOOTPRINT
C0402
PARTTYPE
CL05B104KB54PNC
DESCRIPTION
容值:100nF;精度:±10%;额定电压:50V;温度系数:X7R;
Component Kind
Standard
Add into BOM
yes
Convert to PCB
yes
Symbol
CL05B104KB54PNC
Designator
C15
Device
CL05B104KB54PNC
Unique ID
gge9_0
Name
100nF
Reuse Block

Group ID

Channel ID

LCSC Part Name
100nF ±10% 50V
Supplier Part
C307331
Manufacturer
SAMSUNG(三星)
Manufacturer Part
CL05B104KB54PNC
Supplier Footprint
0402
JLCPCB Part Class
Basic Part
Datasheet
https://item.szlcsc.com/datasheet/CL05B104KB54PNC/291005.html
Supplier
LCSC
3D Model Title
C0402_L1.0-W0.5-H0.5
Value
100nF
Tolerance
±10%
Voltage Rating
50V
Temperature Coefficient
X7R
Description
容值:100nF;精度:±10%;额定电压:50V;温度系数:X7R;

*
]
[
DESIGNATOR
C3
FOOTPRINT
C0603
PARTTYPE
CL10A106MA8NRNC
DESCRIPTION
容值:10uF;精度:±20%;额定电压:25V;温度系数:X5R;
Component Kind
Standard
Add into BOM
yes
Convert to PCB
yes
Symbol
CL10A106MA8NRNC
Designator
C3
Device
CL10A106MA8NRNC
Unique ID
gge41_0
LCSC Part Name
10uF ±20% 25V
Supplier Part
C96446
Manufacturer
SAMSUNG(三星)
Manufacturer Part
CL10A106MA8NRNC
Supplier Footprint
0603
JLCPCB Part Class
Basic Part
Datasheet
https://item.szlcsc.com/datasheet/CL10A106MA8NRNC/97651.html
Supplier
LCSC
3D Model Title
C0603_L1.6-W0.8-H0.8
Value
10uF
Tolerance
±20%
Voltage Rating
25V
Temperature Coefficient
X5R
Name
10uF
Description
容值:10uF;精度:±20%;额定电压:25V;温度系数:X5R;
Reuse Block

Group ID

Channel ID


*
]
[
DESIGNATOR
C18
FOOTPRINT
C0402
PARTTYPE
CL05B104KB54PNC
DESCRIPTION
容值:100nF;精度:±10%;额定电压:50V;温度系数:X7R;
Component Kind
Standard
Add into BOM
yes
Convert to PCB
yes
Symbol
CL05B104KB54PNC
Designator
C18
Device
CL05B104KB54PNC
Unique ID
gge9_1
Name
100nF
Reuse Block

Group ID

Channel ID

LCSC Part Name
100nF ±10% 50V
Supplier Part
C307331
Manufacturer
SAMSUNG(三星)
Manufacturer Part
CL05B104KB54PNC
Supplier Footprint
0402
JLCPCB Part Class
Basic Part
Datasheet
https://item.szlcsc.com/datasheet/CL05B104KB54PNC/291005.html
Supplier
LCSC
3D Model Title
C0402_L1.0-W0.5-H0.5
Value
100nF
Tolerance
±10%
Voltage Rating
50V
Temperature Coefficient
X7R
Description
容值:100nF;精度:±10%;额定电压:50V;温度系数:X7R;

*
]
[
DESIGNATOR
L2
FOOTPRINT
L0603
PARTTYPE
BLM18PG121SN1D
DESCRIPTION
阻抗@频率:120Ω@100MHz;误差:±25%;直流电阻(DCR):50mΩ;
Component Kind
Standard
Add into BOM
yes
Convert to PCB
yes
Symbol
BLM18PG121SN1D_C14709
Designator
L2
Device
BLM18PG121SN1D
Unique ID
gge89
Name
BLM18PG121SN1D
Reuse Block

Group ID

Channel ID

LCSC Part Name
单路 0603磁珠 阻抗120Ω@100MHz
Supplier Part
C14709
Manufacturer
muRata(村田)
Manufacturer Part
BLM18PG121SN1D
Supplier Footprint
0603
JLCPCB Part Class
Basic Part
Datasheet
https://item.szlcsc.com/datasheet/BLM18PG121SN1D/15379.html
Supplier
LCSC
3D Model Title
L0603_L1.6-W0.8-H0.5_BEAD
Impedance @ Frequency
120Ω@100MHz
Tolerance
±25%
DC Resistance(DCR)
50mΩ
Current Rating
2A
Number of Circuits
1
Operating Temperature
-55℃~+125℃
Description
阻抗@频率:120Ω@100MHz;误差:±25%;直流电阻(DCR):50mΩ;

*
]
[
DESIGNATOR
C19
FOOTPRINT
C0402
PARTTYPE
CL05B104KB54PNC
DESCRIPTION
容值:100nF;精度:±10%;额定电压:50V;温度系数:X7R;
Component Kind
Standard
Add into BOM
yes
Convert to PCB
yes
Symbol
CL05B104KB54PNC
Designator
C19
Device
CL05B104KB54PNC
Unique ID
gge9_2
Name
100nF
Reuse Block

Group ID

Channel ID

LCSC Part Name
100nF ±10% 50V
Supplier Part
C307331
Manufacturer
SAMSUNG(三星)
Manufacturer Part
CL05B104KB54PNC
Supplier Footprint
0402
JLCPCB Part Class
Basic Part
Datasheet
https://item.szlcsc.com/datasheet/CL05B104KB54PNC/291005.html
Supplier
LCSC
3D Model Title
C0402_L1.0-W0.5-H0.5
Value
100nF
Tolerance
±10%
Voltage Rating
50V
Temperature Coefficient
X7R
Description
容值:100nF;精度:±10%;额定电压:50V;温度系数:X7R;

*
]
[
DESIGNATOR
C20
FOOTPRINT
C0402
PARTTYPE
CL05B104KB54PNC
DESCRIPTION
容值:100nF;精度:±10%;额定电压:50V;温度系数:X7R;
Component Kind
Standard
Add into BOM
yes
Convert to PCB
yes
Symbol
CL05B104KB54PNC
Designator
C20
Device
CL05B104KB54PNC
Unique ID
gge92
Name
100nF
Reuse Block

Group ID

Channel ID

LCSC Part Name
100nF ±10% 50V
Supplier Part
C307331
Manufacturer
SAMSUNG(三星)
Manufacturer Part
CL05B104KB54PNC
Supplier Footprint
0402
JLCPCB Part Class
Basic Part
Datasheet
https://item.szlcsc.com/datasheet/CL05B104KB54PNC/291005.html
Supplier
LCSC
3D Model Title
C0402_L1.0-W0.5-H0.5
Value
100nF
Tolerance
±10%
Voltage Rating
50V
Temperature Coefficient
X7R
Description
容值:100nF;精度:±10%;额定电压:50V;温度系数:X7R;

*
]
[
DESIGNATOR
C21
FOOTPRINT
C0402
PARTTYPE
CL05B104KB54PNC
DESCRIPTION
容值:100nF;精度:±10%;额定电压:50V;温度系数:X7R;
Component Kind
Standard
Add into BOM
yes
Convert to PCB
yes
Symbol
CL05B104KB54PNC
Designator
C21
Device
CL05B104KB54PNC
Unique ID
gge9_3
Name
100nF
Reuse Block

Group ID

Channel ID

LCSC Part Name
100nF ±10% 50V
Supplier Part
C307331
Manufacturer
SAMSUNG(三星)
Manufacturer Part
CL05B104KB54PNC
Supplier Footprint
0402
JLCPCB Part Class
Basic Part
Datasheet
https://item.szlcsc.com/datasheet/CL05B104KB54PNC/291005.html
Supplier
LCSC
3D Model Title
C0402_L1.0-W0.5-H0.5
Value
100nF
Tolerance
±10%
Voltage Rating
50V
Temperature Coefficient
X7R
Description
容值:100nF;精度:±10%;额定电压:50V;温度系数:X7R;

*
]
[
DESIGNATOR
C22
FOOTPRINT
C0402
PARTTYPE
CL05B104KB54PNC
DESCRIPTION
容值:100nF;精度:±10%;额定电压:50V;温度系数:X7R;
Component Kind
Standard
Add into BOM
yes
Convert to PCB
yes
Symbol
CL05B104KB54PNC
Designator
C22
Device
CL05B104KB54PNC
Unique ID
gge9_4
Name
100nF
Reuse Block

Group ID

Channel ID

LCSC Part Name
100nF ±10% 50V
Supplier Part
C307331
Manufacturer
SAMSUNG(三星)
Manufacturer Part
CL05B104KB54PNC
Supplier Footprint
0402
JLCPCB Part Class
Basic Part
Datasheet
https://item.szlcsc.com/datasheet/CL05B104KB54PNC/291005.html
Supplier
LCSC
3D Model Title
C0402_L1.0-W0.5-H0.5
Value
100nF
Tolerance
±10%
Voltage Rating
50V
Temperature Coefficient
X7R
Description
容值:100nF;精度:±10%;额定电压:50V;温度系数:X7R;

*
]
[
DESIGNATOR
U4
FOOTPRINT
ESOP-8_L4.9-W3.9-P1.27-LS6.0-BL-EP
PARTTYPE
IP5306
DESCRIPTION
工作电压:4.65V~5.5V;最大充电电流:2.1A;电池类型:锂电池;电池节数:1;
Component Kind
Standard
Add into BOM
yes
Convert to PCB
yes
Symbol
IP5306
Designator
U4
Device
IP5306
Unique ID
gge93
Name
IP5306
Reuse Block

Group ID

Channel ID

LCSC Part Name
集成2.1A充电器和2.1A放电器的移动电源系统级芯片
Supplier Part
C181692
Manufacturer
INJOINIC(英集芯)
Manufacturer Part
IP5306
Supplier Footprint
ESOP-8
JLCPCB Part Class
Extended Part
Datasheet
https://item.szlcsc.com/datasheet/IP5306/193089.html
Supplier
LCSC
3D Model Title
ESOP-8_L4.9-W3.9-H1.6-LS6.0-P1.27
The Chip Type
充电芯片；保护芯片
Voltage - Supply
4.65V~5.5V
Charge Current - Max
2.1A
Charging Saturation Voltage
4.2V
End-Off Voltage
3V
Type of Battery
锂电池
Number of Cells
1
Operating Temperature
0℃~+70℃
Battery Temperature Detection
不支持
0V Battery Charge
不支持
Supply Current (Iq)
100uA
Balance Current
-
Interface
I2C
Features
过流保护；恒流充电；自动再充电；充电终止；过压保护；欠压锁定；过放保护；涓流充电；短路保护
Description
工作电压:4.65V~5.5V;最大充电电流:2.1A;电池类型:锂电池;电池节数:1;

*
]
[
DESIGNATOR
J6
FOOTPRINT
CONN-TH_B4B-XH-A-LF-SN
PARTTYPE
B4B-XH-A(LF)(SN)
DESCRIPTION
插针结构:1x4P;间距:2.5mm;安装方式:直插;参考系列:XH;总PIN数:4P;排数:1;每排PIN数:4;行距:-;额定电流:3A;触头材质:黄铜;触头镀层:锡;工作温度:-25℃~+85℃;
Component Kind
Standard
Add into BOM
yes
Convert to PCB
yes
Symbol
B4B-XH-A(LF)(SN)
Designator
J6
Device
B4B-XH-A(LF)(SN)
Unique ID
gge94
Name
B4B-XH-A(LF)(SN)
Reuse Block

Group ID

Channel ID

LCSC Part Name
1x4P 间距:2.5mm 直插 系列:XH
Supplier Part
C144395
Manufacturer
JST
Manufacturer Part
B4B-XH-A(LF)(SN)
Supplier Footprint
插件,P=2.5mm
JLCPCB Part Class
Extended Part
Datasheet
https://item.szlcsc.com/datasheet/B4B-XH-A(LF)(SN)/155727.html
Supplier
LCSC
3D Model Title
XH2.5-4A
Pins Structure
1x4P
Pitch
2.5mm
Mounting Type
直插
Reference Series
XH
Number of Pins
4P
Number of Rows
1
Number of PINs Per Row
4
Row Spacing
-
Current Rating
3A
Contact Material
黄铜
Contact Plating
锡
Operating Temperature
-25℃~+85℃
Voltage Rating
250V
Plastic Material
PA66
Flame Retardant Rating
UL94V-0
Supplementary Features
打K脚
Color
白色
Z-Height of the Board
7mm
X-Length of Bottom Edge on Board (Spacing Line)
12.4mm
Y-Width of Bottom Edge on Board
5.75mm
Description
插针结构:1x4P;间距:2.5mm;安装方式:直插;参考系列:XH;总PIN数:4P;排数:1;每排PIN数:4;行距:-;额定电流:3A;触头材质:黄铜;触头镀层:锡;工作温度:-25℃~+85℃;

*
]
[
DESIGNATOR
J3
FOOTPRINT
CONN-TH_B2B-XH-A-LF-SN
PARTTYPE
B2B-XH-A(LF)(SN)
DESCRIPTION
插针结构:1x2P;间距:2.5mm;安装方式:直插;参考系列:XH;总PIN数:2P;排数:1;每排PIN数:2;行距:-;额定电流:3A;触头材质:黄铜;触头镀层:锡;工作温度:-25℃~+85℃;
Component Kind
Standard
Add into BOM
yes
Convert to PCB
yes
Symbol
B2B-XH-A (LF)(SN)
Designator
J3
Device
B2B-XH-A(LF)(SN)
Unique ID
gge32_0
Name
B2B-XH-A(LF)(SN)
Reuse Block

Group ID

Channel ID

LCSC Part Name
1x2P 间距:2.5mm 直插 系列:XH
Supplier Part
C158012
Manufacturer
JST
Manufacturer Part
B2B-XH-A(LF)(SN)
Supplier Footprint
插件,P=2.5mm
JLCPCB Part Class
Extended Part
Datasheet
https://item.szlcsc.com/datasheet/B2B-XH-A(LF)(SN)/169360.html
Supplier
LCSC
3D Model Title
XH2.5-2A
Pins Structure
1x2P
Pitch
2.5mm
Mounting Type
直插
Reference Series
XH
Number of Pins
2P
Number of Rows
1
Number of PINs Per Row
2
Row Spacing
-
Current Rating
3A
Contact Material
黄铜
Contact Plating
锡
Operating Temperature
-25℃~+85℃
Voltage Rating
250V
Plastic Material
PA66
Flame Retardant Rating
UL94V-0
Supplementary Features
打K脚
Color
白色
Z-Height of the Board
7mm
X-Length of Bottom Edge on Board (Spacing Line)
7.4mm
Y-Width of Bottom Edge on Board
5.75mm
Description
插针结构:1x2P;间距:2.5mm;安装方式:直插;参考系列:XH;总PIN数:2P;排数:1;每排PIN数:2;行距:-;额定电流:3A;触头材质:黄铜;触头镀层:锡;工作温度:-25℃~+85℃;

*
]
[
DESIGNATOR
SPK1
FOOTPRINT
BUZ-SMD_4P-L13.0-W13.0-P11.4-BL
PARTTYPE
FS-1340
DESCRIPTION
阻抗:8Ω;谐振频率:850Hz;失真(THD):5%;额定功率:700mW;声压(SPL):88dB;
Component Kind
Standard
Add into BOM
yes
Convert to PCB
yes
Symbol
FS-1340
Designator
SPK1
Device
FS-1340
Unique ID
gge95
Name
FS-1340
Reuse Block

Group ID

Channel ID

LCSC Part Name
喇叭13*13MM-4.0H 8Ω0.5W 贴片
Supplier Part
C482342
Manufacturer
FUET(福声科技)
Manufacturer Part
FS-1340
Supplier Footprint
-
JLCPCB Part Class
Extended Part
Datasheet
https://item.szlcsc.com/datasheet/FS-1340/490268.html
Supplier
LCSC
3D Model Title
BUZ-SMD_4P-L13.0-W13.0-P11.4-BL
Frequency Range
850Hz~20kHz
Impedance
8Ω
Resonant Frequency
850Hz
Total Harmonic Distortion(THD)
5%
Rated Power
700mW
Sound Pressure Level(SPL)
88dB
Length
13mm
Width
13mm
Height
4mm
Operating Temperature
-40℃~+85℃
Mounting Type
贴片
Description
阻抗:8Ω;谐振频率:850Hz;失真(THD):5%;额定功率:700mW;声压(SPL):88dB;

*
]
[
DESIGNATOR
R2
FOOTPRINT
R0402
PARTTYPE
0402WGF1001TCE
DESCRIPTION
电阻类型:厚膜电阻;阻值:1kΩ;精度:±1%;功率:62.5mW;工作电压:50V;温度系数:±100ppm/℃;
Component Kind
Standard
Add into BOM
yes
Convert to PCB
yes
Symbol
0402WGF1001TCE
Designator
R2
Device
0402WGF1001TCE
Unique ID
gge96
Name
1kΩ
Reuse Block

Group ID

Channel ID

LCSC Part Name
1kΩ ±1% 62.5mW 厚膜电阻
Supplier Part
C11702
Manufacturer
UNI-ROYAL(厚声)
Manufacturer Part
0402WGF1001TCE
Supplier Footprint
0402
JLCPCB Part Class
Basic Part
Datasheet
https://item.szlcsc.com/datasheet/0402WGF1001TCE/12256.html
Supplier
LCSC
3D Model Title
R0402_L1.0-W0.5-H0.4
Type
厚膜电阻
Value
1kΩ
Tolerance
±1%
Power(Watts)
62.5mW
Voltage-Supply(Max)
50V
Temperature Coefficient
±100ppm/℃
Operating Temperature
-55℃~+155℃
Description
电阻类型:厚膜电阻;阻值:1kΩ;精度:±1%;功率:62.5mW;工作电压:50V;温度系数:±100ppm/℃;

*
]
[
DESIGNATOR
L3
FOOTPRINT
IND-SMD_L4.4-W4.2
PARTTYPE
FXL0420-1R0-M
DESCRIPTION
电感值:1uH;精度:±20%;额定电流:6A;饱和电流(Isat):7A;类型:一体成型电感;
Component Kind
Standard
Add into BOM
yes
Convert to PCB
yes
Symbol
FXL0420-1R0-M
Designator
L3
Device
FXL0420-1R0-M
Unique ID
gge97
Name
1uH
Reuse Block

Group ID

Channel ID

LCSC Part Name
1uH ±20% 7A
Supplier Part
C167203
Manufacturer
cjiang(长江微电)
Manufacturer Part
FXL0420-1R0-M
Supplier Footprint
SMD,4.2x4.4mm
JLCPCB Part Class
Extended Part
Datasheet
https://atta.szlcsc.com/upload/public/pdf/source/20240426/3189EA8206330E2108542F9E34E540E7.pdf
Supplier
LCSC
3D Model Title
IND-SMD_L4.2-W4.4-H2.0
Value
1uH
Tolerance
±20%
Rated Current
6A
Saturation Current (Isat)
7A
DC Resistance (DCR)
27mΩ
Type
一体成型电感
Description
电感值:1uH;精度:±20%;额定电流:6A;饱和电流(Isat):7A;类型:一体成型电感;

*
]
[
DESIGNATOR
R8
FOOTPRINT
R0603
PARTTYPE
0603WAF0000T5E
DESCRIPTION
电阻类型:厚膜电阻;阻值:0Ω;精度:±1%;功率:100mW;工作电压:75V;温度系数:-;
Component Kind
Standard
Add into BOM
yes
Convert to PCB
yes
Symbol
0603WAF0000T5E
Designator
R8
Device
0603WAF0000T5E
Unique ID
gge101
Name
0Ω
Reuse Block

Group ID

Channel ID

LCSC Part Name
0Ω ±1% 100mW 厚膜电阻
Supplier Part
C21189
Manufacturer
UNI-ROYAL(厚声)
Manufacturer Part
0603WAF0000T5E
Supplier Footprint
0603
JLCPCB Part Class
Basic Part
Datasheet
https://item.szlcsc.com/datasheet/0603WAF0000T5E/21903.html
Supplier
LCSC
3D Model Title
R0603
Type
厚膜电阻
Value
0Ω
Tolerance
±1%
Power(Watts)
100mW
Voltage-Supply(Max)
75V
Temperature Coefficient
-
Operating Temperature
-55℃~+155℃
Description
电阻类型:厚膜电阻;阻值:0Ω;精度:±1%;功率:100mW;工作电压:75V;温度系数:-;

*
]
[
DESIGNATOR
R13
FOOTPRINT
R0402
PARTTYPE
0402WGF4702TCE
DESCRIPTION
电阻类型:厚膜电阻;阻值:47kΩ;精度:±1%;功率:62.5mW;工作电压:50V;温度系数:±100ppm/℃;
Component Kind
Standard
Add into BOM
yes
Convert to PCB
yes
Symbol
0402WGF4702TCE
Designator
R13
Device
0402WGF4702TCE
Unique ID
gge102
Name
47kΩ
Reuse Block

Group ID

Channel ID

LCSC Part Name
47kΩ ±1% 62.5mW 厚膜电阻
Supplier Part
C25792
Manufacturer
UNI-ROYAL(厚声)
Manufacturer Part
0402WGF4702TCE
Supplier Footprint
0402
JLCPCB Part Class
Basic Part
Datasheet
https://item.szlcsc.com/datasheet/0402WGF4702TCE/26535.html
Supplier
LCSC
3D Model Title
R0402_L1.0-W0.5-H0.4
Type
厚膜电阻
Value
47kΩ
Tolerance
±1%
Power(Watts)
62.5mW
Voltage-Supply(Max)
50V
Temperature Coefficient
±100ppm/℃
Operating Temperature
-55℃~+155℃
Description
电阻类型:厚膜电阻;阻值:47kΩ;精度:±1%;功率:62.5mW;工作电压:50V;温度系数:±100ppm/℃;

*
]
[
DESIGNATOR
C25
FOOTPRINT
C0603
PARTTYPE
CL10A106KP8NNNC
DESCRIPTION
容值:10uF;精度:±10%;额定电压:10V;温度系数:X5R;
Component Kind
Standard
Add into BOM
yes
Convert to PCB
yes
Symbol
CL10A106KP8NNNC
Designator
C25
Device
CL10A106KP8NNNC
Unique ID
gge105
Name
10uF
Reuse Block

Group ID

Channel ID

LCSC Part Name
10uF ±10% 10V
Supplier Part
C19702
Manufacturer
SAMSUNG(三星)
Manufacturer Part
CL10A106KP8NNNC
Supplier Footprint
0603
JLCPCB Part Class
Basic Part
Datasheet
https://item.szlcsc.com/datasheet/CL10A106KP8NNNC/20411.html
Supplier
LCSC
3D Model Title
C0603_L1.6-W0.8-H0.8
Value
10uF
Tolerance
±10%
Voltage Rating
10V
Temperature Coefficient
X5R
Description
容值:10uF;精度:±10%;额定电压:10V;温度系数:X5R;

*
]
[
DESIGNATOR
C23
FOOTPRINT
C0603
PARTTYPE
CL10A106KP8NNNC
DESCRIPTION
容值:10uF;精度:±10%;额定电压:10V;温度系数:X5R;
Component Kind
Standard
Add into BOM
yes
Convert to PCB
yes
Symbol
CL10A106KP8NNNC
Designator
C23
Device
CL10A106KP8NNNC
Unique ID
gge107
Name
10uF
Reuse Block

Group ID

Channel ID

LCSC Part Name
10uF ±10% 10V
Supplier Part
C19702
Manufacturer
SAMSUNG(三星)
Manufacturer Part
CL10A106KP8NNNC
Supplier Footprint
0603
JLCPCB Part Class
Basic Part
Datasheet
https://item.szlcsc.com/datasheet/CL10A106KP8NNNC/20411.html
Supplier
LCSC
3D Model Title
C0603_L1.6-W0.8-H0.8
Value
10uF
Tolerance
±10%
Voltage Rating
10V
Temperature Coefficient
X5R
Description
容值:10uF;精度:±10%;额定电压:10V;温度系数:X5R;

*
]
[
DESIGNATOR
D3
FOOTPRINT
SOD-123FL_L2.7-W1.8-LS3.8-RD
PARTTYPE
SMF5.0A_C19077497
DESCRIPTION
极性:单向;反向截止电压(Vrwm):5V;钳位电压:9.2V;峰值脉冲电流(Ipp):21.7A@10/1000us;峰值脉冲功率(Ppp):200W@10/1000us;击穿电压:7V;
Component Kind
Standard
Add into BOM
yes
Convert to PCB
yes
Symbol
SMF5.0A_C19077497
Designator
D3
Device
SMF5.0A_C19077497
Unique ID
gge108
Name
SMF5.0A
Reuse Block

Group ID

Channel ID

LCSC Part Name
单向TVS 5V截止 峰值浪涌电流：21.7A@10/1000us
Supplier Part
C19077497
Manufacturer
R+O(宏嘉诚)
Manufacturer Part
SMF5.0A
Supplier Footprint
SOD-123FL
JLCPCB Part Class
Extended Part
Datasheet
https://item.szlcsc.com/datasheet/SMF5.0A/20275582.html
Supplier
LCSC
3D Model Title
SOD-123FL_L2.8-W1.8-H1.1-LS3.6
Polarity
单向
Reverse Stand-Off Voltage (Vrwm)
5V
Clamping Voltage
9.2V
Peak Pulse Current (Ipp)
21.7A@10/1000us
Peak Pulse Power Dissipation (Ppp)
200W@10/1000us
Voltage - Breakdown
7V
Reverse Leakage Current (Ir)
400uA
Number of Channels
单路
Operating Temperature
-55℃~+150℃
level of protection
IEC 61000-4-2
Type
TVS
Junction Capacitance
-
Description
极性:单向;反向截止电压(Vrwm):5V;钳位电压:9.2V;峰值脉冲电流(Ipp):21.7A@10/1000us;峰值脉冲功率(Ppp):200W@10/1000us;击穿电压:7V;

*
]
[
DESIGNATOR
R14
FOOTPRINT
R0402
PARTTYPE
0402WGF1002TCE
DESCRIPTION
电阻类型:厚膜电阻;阻值:10kΩ;精度:±1%;功率:62.5mW;工作电压:50V;温度系数:±100ppm/℃;
Component Kind
Standard
Add into BOM
yes
Convert to PCB
yes
Symbol
0402WGF1002TCE
Designator
R14
Device
0402WGF1002TCE
Unique ID
gge109
LCSC Part Name
10kΩ ±1% 62.5mW 厚膜电阻
Supplier Part
C25744
Manufacturer
UNI-ROYAL(厚声)
Manufacturer Part
0402WGF1002TCE
Supplier Footprint
0402
JLCPCB Part Class
Basic Part
Datasheet
https://item.szlcsc.com/datasheet/0402WGF1002TCE/26487.html
Supplier
LCSC
3D Model Title
R0402_L1.0-W0.5-H0.4
Type
厚膜电阻
Value
10kΩ
Tolerance
±1%
Power(Watts)
62.5mW
Voltage-Supply(Max)
50V
Temperature Coefficient
±100ppm/℃
Operating Temperature
-55℃~+155℃
Name
10kΩ
Description
电阻类型:厚膜电阻;阻值:10kΩ;精度:±1%;功率:62.5mW;工作电压:50V;温度系数:±100ppm/℃;
Reuse Block

Group ID

Channel ID


*
]
[
DESIGNATOR
R15
FOOTPRINT
R0402
PARTTYPE
0402WGF1002TCE
DESCRIPTION
电阻类型:厚膜电阻;阻值:10kΩ;精度:±1%;功率:62.5mW;工作电压:50V;温度系数:±100ppm/℃;
Component Kind
Standard
Add into BOM
yes
Convert to PCB
yes
Symbol
0402WGF1002TCE
Designator
R15
Device
0402WGF1002TCE
Unique ID
gge110
LCSC Part Name
10kΩ ±1% 62.5mW 厚膜电阻
Supplier Part
C25744
Manufacturer
UNI-ROYAL(厚声)
Manufacturer Part
0402WGF1002TCE
Supplier Footprint
0402
JLCPCB Part Class
Basic Part
Datasheet
https://item.szlcsc.com/datasheet/0402WGF1002TCE/26487.html
Supplier
LCSC
3D Model Title
R0402_L1.0-W0.5-H0.4
Type
厚膜电阻
Value
10kΩ
Tolerance
±1%
Power(Watts)
62.5mW
Voltage-Supply(Max)
50V
Temperature Coefficient
±100ppm/℃
Operating Temperature
-55℃~+155℃
Name
10kΩ
Description
电阻类型:厚膜电阻;阻值:10kΩ;精度:±1%;功率:62.5mW;工作电压:50V;温度系数:±100ppm/℃;
Reuse Block

Group ID

Channel ID


*
]
[
DESIGNATOR
C24
FOOTPRINT
C0805
PARTTYPE
CL21A226MAQNNNE
DESCRIPTION
容值:22uF;精度:±20%;额定电压:25V;温度系数:X5R;
Component Kind
Standard
Unique ID
gge111
Add into BOM
yes
Convert to PCB
yes
Symbol
CL21A226MAQNNNE
Designator
C24
Device
CL21A226MAQNNNE
LCSC Part Name
22uF ±20% 25V
Supplier Part
C45783
Manufacturer
SAMSUNG(三星)
Manufacturer Part
CL21A226MAQNNNE
Supplier Footprint
0805
JLCPCB Part Class
Basic Part
Datasheet
https://item.szlcsc.com/datasheet/CL21A226MAQNNNE/46786.html
Supplier
LCSC
3D Model Title
C0805_L2.0-W1.3-H1.3
Value
22uF
Tolerance
±20%
Voltage Rating
25V
Temperature Coefficient
X5R
Name
22uF
Description
容值:22uF;精度:±20%;额定电压:25V;温度系数:X5R;
Reuse Block

Group ID

Channel ID


*
]
[
DESIGNATOR
C2
FOOTPRINT
C0402
PARTTYPE
CL05A106MQ5NUNC
DESCRIPTION
容值:10uF;精度:±20%;额定电压:6.3V;温度系数:X5R;
Component Kind
Standard
Unique ID
gge112
Add into BOM
yes
Convert to PCB
yes
Symbol
CL05A106MQ5NUNC
Designator
C2
Device
CL05A106MQ5NUNC
LCSC Part Name
10uF ±20% 6.3V
Supplier Part
C15525
Manufacturer
SAMSUNG(三星)
Manufacturer Part
CL05A106MQ5NUNC
Supplier Footprint
0402
JLCPCB Part Class
Basic Part
Datasheet
https://item.szlcsc.com/datasheet/CL05A106MQ5NUNC/16204.html
Supplier
LCSC
3D Model Title
C0402_L1.0-W0.5-H0.5
Value
10uF
Tolerance
±20%
Voltage Rating
6.3V
Temperature Coefficient
X5R
Name
10uF
Description
容值:10uF;精度:±20%;额定电压:6.3V;温度系数:X5R;
Reuse Block

Group ID

Channel ID


*
]
(
GND 
U2-1 ME6211A33PG-N-VSS Passive 
U5-5 LIS3DHTR-GND Passive 
U5-7 LIS3DHTR-SDO/SA0 Passive 
U5-10 LIS3DHTR-RES Passive 
U5-12 LIS3DHTR-GND Passive 
U3-3 MAX98357AETE+T-GND Passive 
U3-11 MAX98357AETE+T-GND Passive 
U3-15 MAX98357AETE+T-GND Passive 
U3-17 MAX98357AETE+T-EP Passive 
C7-1 CC0603KRX7R9BB104-1 Passive 
C8-1 CL10A106MA8NRNC-1 Passive 
C10-2 CL05B104KO5NNNC-2 Passive 
C12-2 CL05B104KO5NNNC-2 Passive 
R7-1 0402WGF5101TCE-1 Input   
R6-2 0402WGF5101TCE-2 Input   
C13-2 CL05B104KO5NNNC-2 Passive 
J2-1 B8B-XH-AM(LF)(SN)-1 Passive 
J1-A1B12 TYPE-C 16PIN 2MD(073)-GND Passive 
J1-B1A12 TYPE-C 16PIN 2MD(073)-GND Passive 
C9-2 CL10A106MA8NRNC-2 Passive 
C14-2 CC0603KRX7R9BB104-2 Passive 
C11-2 CL10A106MA8NRNC-2 Passive 
C5-1 CL10A225KO8NNNC-1 Input   
C6-1 CL10A225KO8NNNC-1 Input   
U1-57 ESP32-S3FH4R2-GND Passive 
BOOT-1 TS-1088-AR02016-1 Passive 
RESET-2 TS-1088-AR02016-2 Passive 
C4-1 CL05A105KA5NQNC-1 Passive 
R11-2 0402WGF1002TCE-2 Input   
R12-2 0402WGF1002TCE-2 Input   
C16-2 0402CG220J500NT-2 Input   
C17-2 0402CG220J500NT-2 Input   
X1-4 TXM40M0004252HBCEO00T-4 Passive 
X1-2 TXM40M0004252HBCEO00T-2 Passive 
C1-2 CL05B104KB54PNC-2 Passive 
C15-2 CL05B104KB54PNC-2 Passive 
C3-1 CL10A106MA8NRNC-1 Passive 
C18-2 CL05B104KB54PNC-2 Passive 
C19-2 CL05B104KB54PNC-2 Passive 
C20-2 CL05B104KB54PNC-2 Passive 
C21-2 CL05B104KB54PNC-2 Passive 
C22-2 CL05B104KB54PNC-2 Passive 
U4-9 IP5306-EP Passive 
J6-3 B4B-XH-A(LF)(SN)-3 Passive 
J3-2 B2B-XH-A(LF)(SN)-2 Passive 
SPK1-3 FS-1340-3 Passive 
SPK1-4 FS-1340-4 Passive 
R13-2 0402WGF4702TCE-2 Input   
C25-1 CL10A106KP8NNNC-1 Passive 
C23-2 CL10A106KP8NNNC-2 Passive 
D3-2 SMF5.0A_C19077497-A Passive 
R15-2 0402WGF1002TCE-2 Input   
C24-2 CL21A226MAQNNNE-2 Passive 
C2-1 CL05A106MQ5NUNC-1 Input   
)
(
BAT 
U2-2 ME6211A33PG-N-VIN Passive 
C5-2 CL10A225KO8NNNC-2 Input   
U4-6 IP5306-BAT Passive 
J3-1 B2B-XH-A(LF)(SN)-1 Passive 
C25-2 CL10A106KP8NNNC-2 Passive 
R14-2 0402WGF1002TCE-2 Input   
)
(
3V3 
U2-3 ME6211A33PG-N-VOUT Passive 
U5-1 LIS3DHTR-VDD_IO Passive 
U5-8 LIS3DHTR-CS Passive 
U5-14 LIS3DHTR-VDD Passive 
U3-2 MAX98357AETE+T-GAIN_SLOT Passive 
U3-7 MAX98357AETE+T-VDD Passive 
U3-8 MAX98357AETE+T-VDD Passive 
C7-2 CC0603KRX7R9BB104-2 Passive 
C8-2 CL10A106MA8NRNC-2 Passive 
C10-1 CL05B104KO5NNNC-1 Passive 
C12-1 CL05B104KO5NNNC-1 Passive 
C13-1 CL05B104KO5NNNC-1 Passive 
J2-2 B8B-XH-AM(LF)(SN)-2 Passive 
J2-8 B8B-XH-AM(LF)(SN)-8 Passive 
D1-1 KT-0603R-A Passive 
C11-1 CL10A106MA8NRNC-1 Passive 
C6-2 CL10A225KO8NNNC-2 Input   
U1-2 ESP32-S3FH4R2-VDD3P3 Passive 
U1-3 ESP32-S3FH4R2-VDD3P3 Passive 
U1-20 ESP32-S3FH4R2-VDD3P3_RTC Passive 
U1-29 ESP32-S3FH4R2-VDD_SPI Passive 
U1-46 ESP32-S3FH4R2-VDD3P3_CPU Passive 
R1-1 0402WGF1002TCE-1 Input   
R3-1 0402WGF4701TCE-1 Input   
R4-1 0402WGF4701TCE-1 Input   
R5-2 0402WGF1002TCE-2 Input   
C1-1 CL05B104KB54PNC-1 Passive 
C15-1 CL05B104KB54PNC-1 Passive 
C3-2 CL10A106MA8NRNC-2 Passive 
C18-1 CL05B104KB54PNC-1 Passive 
L2-2 BLM18PG121SN1D-2 Passive 
C21-1 CL05B104KB54PNC-1 Passive 
C22-1 CL05B104KB54PNC-1 Passive 
J6-4 B4B-XH-A(LF)(SN)-4 Passive 
)
(
ACCELSCL 
U5-4 LIS3DHTR-SCL/SPC Passive 
U1-23 ESP32-S3FH4R2-GPIO17 Passive 
R3-2 0402WGF4701TCE-2 Input   
)
(
ACCELSDA 
U5-6 LIS3DHTR-SDA/SDI/SDO Passive 
U1-24 ESP32-S3FH4R2-GPIO18 Passive 
R4-2 0402WGF4701TCE-2 Input   
)
(
ACCELINT1 
U5-11 LIS3DHTR-INT1 Passive 
U1-27 ESP32-S3FH4R2-GP1O21 Passive 
)
(
AMPDIN 
U3-1 MAX98357AETE+T-DIN Passive 
U1-12 ESP32-S3FH4R2-GPIO7 Passive 
)
(
AMPSDMODE 
U3-4 MAX98357AETE+T-SD_MODE# Passive 
U1-18 ESP32-S3FH4R2-GPIO13 Passive 
R13-1 0402WGF4702TCE-1 Input   
)
(
SPKP 
U3-9 MAX98357AETE+T-OUTP Passive 
SPK1-1 FS-1340-+ Passive 
)
(
SPKN 
U3-10 MAX98357AETE+T-OUTN Passive 
SPK1-2 FS-1340-- Passive 
)
(
I2SWS 
U3-14 MAX98357AETE+T-LRCLK Passive 
U1-10 ESP32-S3FH4R2-GPIO5 Passive 
)
(
I2SBCLK 
U3-16 MAX98357AETE+T-BCLK Passive 
U1-9 ESP32-S3FH4R2-GPIO4 Passive 
)
(
$1N95 
R7-2 0402WGF5101TCE-2 Input   
J1-B5 TYPE-C 16PIN 2MD(073)-CC2 Passive 
)
(
$1N152 
R6-1 0402WGF5101TCE-1 Input   
J1-A5 TYPE-C 16PIN 2MD(073)-CC1 Passive 
)
(
LCDCLK 
J2-3 B8B-XH-AM(LF)(SN)-3 Passive 
U1-17 ESP32-S3FH4R2-GPIO12 Passive 
)
(
LCDMOSI 
J2-4 B8B-XH-AM(LF)(SN)-4 Passive 
U1-16 ESP32-S3FH4R2-GPIO11 Passive 
)
(
LCDRST 
J2-5 B8B-XH-AM(LF)(SN)-5 Passive 
U1-13 ESP32-S3FH4R2-GPIO8 Passive 
)
(
LCDDC 
J2-6 B8B-XH-AM(LF)(SN)-6 Passive 
U1-14 ESP32-S3FH4R2-GPIO9 Passive 
)
(
LCDCS 
J2-7 B8B-XH-AM(LF)(SN)-7 Passive 
U1-15 ESP32-S3FH4R2-GPIO10 Passive 
)
(
$1N257 
D1-2 KT-0603R-K Passive 
R2-1 0402WGF1001TCE-1 Input   
)
(
$1N173 
J1-A4B9 TYPE-C 16PIN 2MD(073)-VBUS Passive 
J1-B4A9 TYPE-C 16PIN 2MD(073)-VBUS Passive 
R8-2 0603WAF0000T5E-2 Input   
D3-1 SMF5.0A_C19077497-K Passive 
)
(
USBDN 
J1-B7 TYPE-C 16PIN 2MD(073)-Dn2 Passive 
J1-A7 TYPE-C 16PIN 2MD(073)-Dn1 Passive 
R9-1 0402WGF220JTCE-1 Input   
)
(
USBDP 
J1-A6 TYPE-C 16PIN 2MD(073)-Dp1 Passive 
J1-B6 TYPE-C 16PIN 2MD(073)-Dp2 Passive 
R10-1 0402WGF220JTCE-1 Input   
)
(
VBUS 
C9-1 CL10A106MA8NRNC-1 Passive 
C14-1 CC0603KRX7R9BB104-1 Passive 
U4-1 IP5306-VIN Passive 
R8-1 0603WAF0000T5E-1 Input   
C23-1 CL10A106KP8NNNC-1 Passive 
)
(
TOUCHRFACE 
J4-1 B3B-XH-A(LF)(SN)-1 Passive 
U1-11 ESP32-S3FH4R2-GPIO6 Passive 
)
(
TOUCHLFACE 
J4-2 B3B-XH-A(LF)(SN)-2 Passive 
U1-7 ESP32-S3FH4R2-GPIO2 Passive 
)
(
TOUCHHEAD 
J4-3 B3B-XH-A(LF)(SN)-3 Passive 
U1-6 ESP32-S3FH4R2-GPIO1 Passive 
)
(
RESET 
U1-4 ESP32-S3FH4R2-CHIP_PU Passive 
R5-1 0402WGF1002TCE-1 Input   
RESET-1 TS-1088-AR02016-1 Passive 
C4-2 CL05A105KA5NQNC-2 Passive 
)
(
$1N183 
U1-5 ESP32-S3FH4R2-GPIO0 Passive 
R1-2 0402WGF1002TCE-2 Input   
BOOT-2 TS-1088-AR02016-2 Passive 
)
(
BATADC 
U1-19 ESP32-S3FH4R2-GPIO14 Passive 
R14-1 0402WGF1002TCE-1 Input   
R15-1 0402WGF1002TCE-1 Input   
)
(
$1N200 
U1-25 ESP32-S3FH4R2-GPIO19 Passive 
R9-2 0402WGF220JTCE-2 Input   
)
(
$1N199 
U1-26 ESP32-S3FH4R2-GPIO20 Passive 
R10-2 0402WGF220JTCE-2 Input   
)
(
TXD0 
U1-49 ESP32-S3FH4R2-U0TXD Passive 
J6-1 B4B-XH-A(LF)(SN)-1 Passive 
)
(
RXD0 
U1-50 ESP32-S3FH4R2-U0RXD Passive 
J6-2 B4B-XH-A(LF)(SN)-2 Passive 
)
(
$1N216 
U1-51 ESP32-S3FH4R2-GPIO45 Passive 
R12-1 0402WGF1002TCE-1 Input   
)
(
$1N215 
U1-52 ESP32-S3FH4R2-GPIO46 Passive 
R11-1 0402WGF1002TCE-1 Input   
)
(
$1N222 
U1-53 ESP32-S3FH4R2-XTAL_N Passive 
C16-1 0402CG220J500NT-1 Input   
X1-3 TXM40M0004252HBCEO00T-OSC2 Passive 
)
(
$1N221 
U1-54 ESP32-S3FH4R2-XTAL_P Passive 
L1-1 LQW15AN24NG00D-1 Passive 
)
(
$1N236 
U1-55 ESP32-S3FH4R2-VDDA Passive 
U1-56 ESP32-S3FH4R2-VDDA Passive 
L2-1 BLM18PG121SN1D-1 Passive 
C19-1 CL05B104KB54PNC-1 Passive 
C20-1 CL05B104KB54PNC-1 Passive 
C2-2 CL05A106MQ5NUNC-2 Input   
)
(
$1N227 
L1-2 LQW15AN24NG00D-2 Passive 
C17-1 0402CG220J500NT-1 Input   
X1-1 TXM40M0004252HBCEO00T-OSC1 Passive 
)
(
$1N258 
U4-2 IP5306-LED1 Passive 
R2-2 0402WGF1001TCE-2 Input   
)
(
SW 
U4-7 IP5306-SW Passive 
L3-1 FXL0420-1R0-M-1 Passive 
)
(
VOUT 
U4-8 IP5306-VOUT Passive 
L3-2 FXL0420-1R0-M-2 Passive 
C24-1 CL21A226MAQNNNE-1 Passive 
)
