PROTEL NETLIST 2.0
[
DESIGNATOR
BOOT
FOOTPRINT
SW-SMD_L3.9-W3.0-P4.45
PARTTYPE
TS-1088-AR02016
DESCRIPTION
电路结构:单刀单掷;按钮形状:圆形按钮;作用力:1.6N;安装方式:立贴;开关长度:3.9mm;开关宽度:3mm;开关高度:2mm;带支架:不带支架;触点电流:50mA;额定电压:12V;带灯:-;工作寿命:10万次;
Component Kind
Standard
Footprint
SW-SMD_L3.9-W3.0-P4.45
Designator
BOOT
LCSC Part Name
3.9*3*2mm 立贴 轻触开关
Supplier Part
C720477
Manufacturer
XUNPU(讯普)
Manufacturer Part
TS-1088-AR02016
Supplier Footprint
SMD,4x3mm
JLCPCB Part Class
Basic Part
Datasheet
https://item.szlcsc.com/datasheet/TS-1088-AR02016/763484.html
Supplier
LCSC
Add into BOM
yes
3D Model Title
SW-SMD_L3.9-W2.9-H2.0-LS4.8
Circuit
单刀单掷
Actuator Style
圆形按钮
Operating Force
1.6N
Mounting Type
立贴
Length
3.9mm
Width
3mm
Switch Height
2mm
with Bracket
不带支架
Contact Current
50mA
Voltage Rating
12V
Actuator/Cap Color
黑色
With Lamp
-
IP Rating
-
Termination Style
SMD接片
Life
10万次
Operating Temperature
-30℃~+80℃
Name
TS-1088-AR02016
Description
电路结构:单刀单掷;按钮形状:圆形按钮;作用力:1.6N;安装方式:立贴;开关长度:3.9mm;开关宽度:3mm;开关高度:2mm;带支架:不带支架;触点电流:50mA;额定电压:12V;带灯:-;工作寿命:10万次;
Device
TS-1088-AR02016
Unique ID
gge13
Reuse Block

Group ID

Channel ID
$1I109
PCB Layer
TopLayer
Convert to PCB
yes

*
]
[
DESIGNATOR
C1
FOOTPRINT
C0402
PARTTYPE
CL05B104KB54PNC
DESCRIPTION
容值:100nF;精度:±10%;额定电压:50V;温度系数:X7R;
Component Kind
Standard
Footprint
C0402
Designator
C1
LCSC Part Name
100nF ±10% 50V
Supplier Part
C307331
Manufacturer
SAMSUNG(三星)
Manufacturer Part
CL05B104KB54PNC
Supplier Footprint
0402
JLCPCB Part Class
Basic Part
Datasheet
https://item.szlcsc.com/datasheet/CL05B104KB54PNC/291005.html
Supplier
LCSC
Add into BOM
yes
3D Model Title
C0402_L1.0-W0.5-H0.5
Value
100nF
Tolerance
±10%
Voltage Rating
50V
Temperature Coefficient
X7R
Name
100nF
Description
容值:100nF;精度:±10%;额定电压:50V;温度系数:X7R;
Device
CL05B104KB54PNC
Unique ID
gge9
Reuse Block

Group ID

Channel ID
$1I132
PCB Layer
TopLayer
Convert to PCB
yes

*
]
[
DESIGNATOR
C3
FOOTPRINT
C0603
PARTTYPE
CL10A106MA8NRNC
DESCRIPTION
容值:10uF;精度:±20%;额定电压:25V;温度系数:X5R;
Component Kind
Standard
Footprint
C0603
Designator
C3
LCSC Part Name
10uF ±20% 25V
Supplier Part
C96446
Manufacturer
SAMSUNG(三星)
Manufacturer Part
CL10A106MA8NRNC
Supplier Footprint
0603
JLCPCB Part Class
Basic Part
Datasheet
https://item.szlcsc.com/datasheet/CL10A106MA8NRNC/97651.html
Supplier
LCSC
Add into BOM
yes
3D Model Title
C0603_L1.6-W0.8-H0.8
Value
10uF
Tolerance
±20%
Voltage Rating
25V
Temperature Coefficient
X5R
Name
10uF
Description
容值:10uF;精度:±20%;额定电压:25V;温度系数:X5R;
Device
CL10A106MA8NRNC
Unique ID
gge41_0
Reuse Block

Group ID

Channel ID
$1I134
PCB Layer
TopLayer
Convert to PCB
yes

*
]
[
DESIGNATOR
C4
FOOTPRINT
C0402
PARTTYPE
CL05A105KA5NQNC
DESCRIPTION
容值:1uF;精度:±10%;额定电压:25V;温度系数:X5R;
Component Kind
Standard
Footprint
C0402
Designator
C4
LCSC Part Name
1uF ±10% 25V
Supplier Part
C52923
Manufacturer
SAMSUNG(三星)
Manufacturer Part
CL05A105KA5NQNC
Supplier Footprint
0402
JLCPCB Part Class
Basic Part
Datasheet
https://item.szlcsc.com/datasheet/CL05A105KA5NQNC/53938.html
Supplier
LCSC
Add into BOM
yes
3D Model Title
C0402_L1.0-W0.5-H0.5
Value
1uF
Tolerance
±10%
Voltage Rating
25V
Temperature Coefficient
X5R
Name
1uF
Description
容值:1uF;精度:±10%;额定电压:25V;温度系数:X5R;
Device
CL05A105KA5NQNC
Unique ID
gge20
Reuse Block

Group ID

Channel ID
$1I116
PCB Layer
TopLayer
Convert to PCB
yes

*
]
[
DESIGNATOR
C5
FOOTPRINT
C0603
PARTTYPE
CL10A225KO8NNNC
DESCRIPTION
容值:2.2uF;精度:±10%;额定电压:16V;温度系数:X5R;
Component Kind
Standard
Footprint
C0603
Designator
C5
LCSC Part Name
2.2uF ±10% 16V
Supplier Part
C23630
Manufacturer
SAMSUNG(三星)
Manufacturer Part
CL10A225KO8NNNC
Supplier Footprint
0603
JLCPCB Part Class
Basic Part
Datasheet
https://item.szlcsc.com/datasheet/CL10A225KO8NNNC/24366.html
Supplier
LCSC
Add into BOM
yes
3D Model Title
C0603_L1.6-W0.8-H0.8
Value
2.2uF
Tolerance
±10%
Voltage Rating
16V
Temperature Coefficient
X5R
Name
2.2uF
Description
容值:2.2uF;精度:±10%;额定电压:16V;温度系数:X5R;
Device
CL10A225KO8NNNC
Unique ID
gge44
Reuse Block

Group ID

Channel ID
$1I94
PCB Layer
TopLayer
Convert to PCB
yes

*
]
[
DESIGNATOR
C6
FOOTPRINT
C0603
PARTTYPE
CL10A225KO8NNNC
DESCRIPTION
容值:2.2uF;精度:±10%;额定电压:16V;温度系数:X5R;
Component Kind
Standard
Footprint
C0603
Designator
C6
LCSC Part Name
2.2uF ±10% 16V
Supplier Part
C23630
Manufacturer
SAMSUNG(三星)
Manufacturer Part
CL10A225KO8NNNC
Supplier Footprint
0603
JLCPCB Part Class
Basic Part
Datasheet
https://item.szlcsc.com/datasheet/CL10A225KO8NNNC/24366.html
Supplier
LCSC
Add into BOM
yes
3D Model Title
C0603_L1.6-W0.8-H0.8
Value
2.2uF
Tolerance
±10%
Voltage Rating
16V
Temperature Coefficient
X5R
Name
2.2uF
Description
容值:2.2uF;精度:±10%;额定电压:16V;温度系数:X5R;
Device
CL10A225KO8NNNC
Unique ID
gge45
Reuse Block

Group ID

Channel ID
$1I95
PCB Layer
TopLayer
Convert to PCB
yes

*
]
[
DESIGNATOR
C7
FOOTPRINT
C0603
PARTTYPE
CC0603KRX7R9BB104
DESCRIPTION
容值:100nF;精度:±10%;额定电压:50V;温度系数:X7R;
Component Kind
Standard
Footprint
C0603
Designator
C7
LCSC Part Name
100nF ±10% 50V
Supplier Part
C14663
Manufacturer
YAGEO(国巨)
Manufacturer Part
CC0603KRX7R9BB104
Supplier Footprint
0603
JLCPCB Part Class
Basic Part
Datasheet
https://item.szlcsc.com/datasheet/CC0603KRX7R9BB104/15331.html
Supplier
LCSC
Add into BOM
yes
3D Model Title
C0603_L1.6-W0.8-H0.8
Value
100nF
Tolerance
±10%
Voltage Rating
50V
Temperature Coefficient
X7R
Name
100nF
Description
容值:100nF;精度:±10%;额定电压:50V;温度系数:X7R;
Device
CC0603KRX7R9BB104
Unique ID
gge24
Reuse Block

Group ID

Channel ID
$1I37
PCB Layer
TopLayer
Convert to PCB
yes

*
]
[
DESIGNATOR
C8
FOOTPRINT
C0603
PARTTYPE
CL10A106MA8NRNC
DESCRIPTION
容值:10uF;精度:±20%;额定电压:25V;温度系数:X5R;
Component Kind
Standard
Footprint
C0603
Designator
C8
LCSC Part Name
10uF ±20% 25V
Supplier Part
C96446
Manufacturer
SAMSUNG(三星)
Manufacturer Part
CL10A106MA8NRNC
Supplier Footprint
0603
JLCPCB Part Class
Basic Part
Datasheet
https://item.szlcsc.com/datasheet/CL10A106MA8NRNC/97651.html
Supplier
LCSC
Add into BOM
yes
3D Model Title
C0603_L1.6-W0.8-H0.8
Value
10uF
Tolerance
±20%
Voltage Rating
25V
Temperature Coefficient
X5R
Name
10uF
Description
容值:10uF;精度:±20%;额定电压:25V;温度系数:X5R;
Device
CL10A106MA8NRNC
Unique ID
gge25
Reuse Block

Group ID

Channel ID
$1I39
PCB Layer
TopLayer
Convert to PCB
yes

*
]
[
DESIGNATOR
C9
FOOTPRINT
C0603
PARTTYPE
CL10A106MA8NRNC
DESCRIPTION
容值:10uF;精度:±20%;额定电压:25V;温度系数:X5R;
Component Kind
Standard
Footprint
C0603
Designator
C9
LCSC Part Name
10uF ±20% 25V
Supplier Part
C96446
Manufacturer
SAMSUNG(三星)
Manufacturer Part
CL10A106MA8NRNC
Supplier Footprint
0603
JLCPCB Part Class
Basic Part
Datasheet
https://item.szlcsc.com/datasheet/CL10A106MA8NRNC/97651.html
Supplier
LCSC
Add into BOM
yes
3D Model Title
C0603_L1.6-W0.8-H0.8
Value
10uF
Tolerance
±20%
Voltage Rating
25V
Temperature Coefficient
X5R
Name
10uF
Description
容值:10uF;精度:±20%;额定电压:25V;温度系数:X5R;
Device
CL10A106MA8NRNC
Unique ID
gge41
Reuse Block

Group ID

Channel ID
$1I88
PCB Layer
TopLayer
Convert to PCB
yes

*
]
[
DESIGNATOR
C10
FOOTPRINT
C0402
PARTTYPE
CL05B104KO5NNNC
DESCRIPTION
容值:100nF;精度:±10%;额定电压:16V;温度系数:X7R;
Component Kind
Standard
Footprint
C0402
Designator
C10
LCSC Part Name
100nF ±10% 16V
Supplier Part
C1525
Manufacturer
SAMSUNG(三星)
Manufacturer Part
CL05B104KO5NNNC
Supplier Footprint
0402
JLCPCB Part Class
Basic Part
Datasheet
https://item.szlcsc.com/datasheet/CL05B104KO5NNNC/1877.html
Supplier
LCSC
Add into BOM
yes
3D Model Title
C0402_L1.0-W0.5-H0.5
Value
100nF
Tolerance
±10%
Voltage Rating
16V
Temperature Coefficient
X7R
Name
100nF
Description
容值:100nF;精度:±10%;额定电压:16V;温度系数:X7R;
Device
CL05B104KO5NNNC
Unique ID
gge27
Reuse Block

Group ID

Channel ID
$1I45
PCB Layer
TopLayer
Convert to PCB
yes

*
]
[
DESIGNATOR
C11
FOOTPRINT
C0603
PARTTYPE
CL10A106MA8NRNC
DESCRIPTION
容值:10uF;精度:±20%;额定电压:25V;温度系数:X5R;
Component Kind
Standard
Footprint
C0603
Designator
C11
LCSC Part Name
10uF ±20% 25V
Supplier Part
C96446
Manufacturer
SAMSUNG(三星)
Manufacturer Part
CL10A106MA8NRNC
Supplier Footprint
0603
JLCPCB Part Class
Basic Part
Datasheet
https://item.szlcsc.com/datasheet/CL10A106MA8NRNC/97651.html
Supplier
LCSC
Add into BOM
yes
3D Model Title
C0603_L1.6-W0.8-H0.8
Value
10uF
Tolerance
±20%
Voltage Rating
25V
Temperature Coefficient
X5R
Name
10uF
Description
容值:10uF;精度:±20%;额定电压:25V;温度系数:X5R;
Device
CL10A106MA8NRNC
Unique ID
gge41_1
Reuse Block

Group ID

Channel ID
$1I92
PCB Layer
TopLayer
Convert to PCB
yes

*
]
[
DESIGNATOR
C12
FOOTPRINT
C0402
PARTTYPE
CL05B104KO5NNNC
DESCRIPTION
容值:100nF;精度:±10%;额定电压:16V;温度系数:X7R;
Component Kind
Standard
Footprint
C0402
Designator
C12
LCSC Part Name
100nF ±10% 16V
Supplier Part
C1525
Manufacturer
SAMSUNG(三星)
Manufacturer Part
CL05B104KO5NNNC
Supplier Footprint
0402
JLCPCB Part Class
Basic Part
Datasheet
https://item.szlcsc.com/datasheet/CL05B104KO5NNNC/1877.html
Supplier
LCSC
Add into BOM
yes
3D Model Title
C0402_L1.0-W0.5-H0.5
Value
100nF
Tolerance
±10%
Voltage Rating
16V
Temperature Coefficient
X7R
Name
100nF
Description
容值:100nF;精度:±10%;额定电压:16V;温度系数:X7R;
Device
CL05B104KO5NNNC
Unique ID
gge28
Reuse Block

Group ID

Channel ID
$1I49
PCB Layer
TopLayer
Convert to PCB
yes

*
]
[
DESIGNATOR
C13
FOOTPRINT
C0402
PARTTYPE
CL05B104KO5NNNC
DESCRIPTION
容值:100nF;精度:±10%;额定电压:16V;温度系数:X7R;
Component Kind
Standard
Footprint
C0402
Designator
C13
LCSC Part Name
100nF ±10% 16V
Supplier Part
C1525
Manufacturer
SAMSUNG(三星)
Manufacturer Part
CL05B104KO5NNNC
Supplier Footprint
0402
JLCPCB Part Class
Basic Part
Datasheet
https://item.szlcsc.com/datasheet/CL05B104KO5NNNC/1877.html
Supplier
LCSC
Add into BOM
yes
3D Model Title
C0402_L1.0-W0.5-H0.5
Value
100nF
Tolerance
±10%
Voltage Rating
16V
Temperature Coefficient
X7R
Name
100nF
Description
容值:100nF;精度:±10%;额定电压:16V;温度系数:X7R;
Device
CL05B104KO5NNNC
Unique ID
gge31
Reuse Block

Group ID

Channel ID
$1I59
PCB Layer
TopLayer
Convert to PCB
yes

*
]
[
DESIGNATOR
C14
FOOTPRINT
C0603
PARTTYPE
CC0603KRX7R9BB104
DESCRIPTION
容值:100nF;精度:±10%;额定电压:50V;温度系数:X7R;
Component Kind
Standard
Footprint
C0603
Designator
C14
LCSC Part Name
100nF ±10% 50V
Supplier Part
C14663
Manufacturer
YAGEO(国巨)
Manufacturer Part
CC0603KRX7R9BB104
Supplier Footprint
0603
JLCPCB Part Class
Basic Part
Datasheet
https://item.szlcsc.com/datasheet/CC0603KRX7R9BB104/15331.html
Supplier
LCSC
Add into BOM
yes
3D Model Title
C0603_L1.6-W0.8-H0.8
Value
100nF
Tolerance
±10%
Voltage Rating
50V
Temperature Coefficient
X7R
Name
100nF
Description
容值:100nF;精度:±10%;额定电压:50V;温度系数:X7R;
Device
CC0603KRX7R9BB104
Unique ID
gge42
Reuse Block

Group ID

Channel ID
$1I89
PCB Layer
TopLayer
Convert to PCB
yes

*
]
[
DESIGNATOR
C15
FOOTPRINT
C0402
PARTTYPE
CL05B104KB54PNC
DESCRIPTION
容值:100nF;精度:±10%;额定电压:50V;温度系数:X7R;
Component Kind
Standard
Footprint
C0402
Designator
C15
LCSC Part Name
100nF ±10% 50V
Supplier Part
C307331
Manufacturer
SAMSUNG(三星)
Manufacturer Part
CL05B104KB54PNC
Supplier Footprint
0402
JLCPCB Part Class
Basic Part
Datasheet
https://item.szlcsc.com/datasheet/CL05B104KB54PNC/291005.html
Supplier
LCSC
Add into BOM
yes
3D Model Title
C0402_L1.0-W0.5-H0.5
Value
100nF
Tolerance
±10%
Voltage Rating
50V
Temperature Coefficient
X7R
Name
100nF
Description
容值:100nF;精度:±10%;额定电压:50V;温度系数:X7R;
Device
CL05B104KB54PNC
Unique ID
gge9_0
Reuse Block

Group ID

Channel ID
$1I133
PCB Layer
TopLayer
Convert to PCB
yes

*
]
[
DESIGNATOR
C16
FOOTPRINT
C0402
PARTTYPE
0402CG220J500NT
DESCRIPTION
容值:22pF;精度:±5%;额定电压:50V;温度系数:C0G;
Component Kind
Standard
Footprint
C0402
Designator
C16
LCSC Part Name
22pF ±5% 50V
Supplier Part
C1555
Manufacturer
FH(风华)
Manufacturer Part
0402CG220J500NT
Supplier Footprint
0402
JLCPCB Part Class
Basic Part
Datasheet
https://item.szlcsc.com/datasheet/0402CG220J500NT/1907.html
Supplier
LCSC
Add into BOM
yes
3D Model Title
C0402_L1.0-W0.5-H0.5
Value
22pF
Tolerance
±5%
Voltage Rating
50V
Temperature Coefficient
C0G
Name
22pF
Description
容值:22pF;精度:±5%;额定电压:50V;温度系数:C0G;
Device
0402CG220J500NT
Unique ID
gge60
Reuse Block

Group ID

Channel ID
$1I128
PCB Layer
TopLayer
Convert to PCB
yes

*
]
[
DESIGNATOR
C17
FOOTPRINT
C0402
PARTTYPE
0402CG220J500NT
DESCRIPTION
容值:22pF;精度:±5%;额定电压:50V;温度系数:C0G;
Component Kind
Standard
Footprint
C0402
Designator
C17
LCSC Part Name
22pF ±5% 50V
Supplier Part
C1555
Manufacturer
FH(风华)
Manufacturer Part
0402CG220J500NT
Supplier Footprint
0402
JLCPCB Part Class
Basic Part
Datasheet
https://item.szlcsc.com/datasheet/0402CG220J500NT/1907.html
Supplier
LCSC
Add into BOM
yes
3D Model Title
C0402_L1.0-W0.5-H0.5
Value
22pF
Tolerance
±5%
Voltage Rating
50V
Temperature Coefficient
C0G
Name
22pF
Description
容值:22pF;精度:±5%;额定电压:50V;温度系数:C0G;
Device
0402CG220J500NT
Unique ID
gge61
Reuse Block

Group ID

Channel ID
$1I129
PCB Layer
TopLayer
Convert to PCB
yes

*
]
[
DESIGNATOR
C18
FOOTPRINT
C0402
PARTTYPE
CL05B104KB54PNC
DESCRIPTION
容值:100nF;精度:±10%;额定电压:50V;温度系数:X7R;
Component Kind
Standard
Footprint
C0402
Designator
C18
LCSC Part Name
100nF ±10% 50V
Supplier Part
C307331
Manufacturer
SAMSUNG(三星)
Manufacturer Part
CL05B104KB54PNC
Supplier Footprint
0402
JLCPCB Part Class
Basic Part
Datasheet
https://item.szlcsc.com/datasheet/CL05B104KB54PNC/291005.html
Supplier
LCSC
Add into BOM
yes
3D Model Title
C0402_L1.0-W0.5-H0.5
Value
100nF
Tolerance
±10%
Voltage Rating
50V
Temperature Coefficient
X7R
Name
100nF
Description
容值:100nF;精度:±10%;额定电压:50V;温度系数:X7R;
Device
CL05B104KB54PNC
Unique ID
gge9_1
Reuse Block

Group ID

Channel ID
$1I138
PCB Layer
TopLayer
Convert to PCB
yes

*
]
[
DESIGNATOR
C19
FOOTPRINT
C0402
PARTTYPE
CL05B104KB54PNC
DESCRIPTION
容值:100nF;精度:±10%;额定电压:50V;温度系数:X7R;
Component Kind
Standard
Footprint
C0402
Designator
C19
LCSC Part Name
100nF ±10% 50V
Supplier Part
C307331
Manufacturer
SAMSUNG(三星)
Manufacturer Part
CL05B104KB54PNC
Supplier Footprint
0402
JLCPCB Part Class
Basic Part
Datasheet
https://item.szlcsc.com/datasheet/CL05B104KB54PNC/291005.html
Supplier
LCSC
Add into BOM
yes
3D Model Title
C0402_L1.0-W0.5-H0.5
Value
100nF
Tolerance
±10%
Voltage Rating
50V
Temperature Coefficient
X7R
Name
100nF
Description
容值:100nF;精度:±10%;额定电压:50V;温度系数:X7R;
Device
CL05B104KB54PNC
Unique ID
gge9_2
Reuse Block

Group ID

Channel ID
$1I143
PCB Layer
TopLayer
Convert to PCB
yes

*
]
[
DESIGNATOR
C20
FOOTPRINT
C0402
PARTTYPE
CL05B104KB54PNC
DESCRIPTION
容值:100nF;精度:±10%;额定电压:50V;温度系数:X7R;
Component Kind
Standard
Footprint
C0402
Designator
C20
LCSC Part Name
100nF ±10% 50V
Supplier Part
C307331
Manufacturer
SAMSUNG(三星)
Manufacturer Part
CL05B104KB54PNC
Supplier Footprint
0402
JLCPCB Part Class
Basic Part
Datasheet
https://item.szlcsc.com/datasheet/CL05B104KB54PNC/291005.html
Supplier
LCSC
Add into BOM
yes
3D Model Title
C0402_L1.0-W0.5-H0.5
Value
100nF
Tolerance
±10%
Voltage Rating
50V
Temperature Coefficient
X7R
Name
100nF
Description
容值:100nF;精度:±10%;额定电压:50V;温度系数:X7R;
Device
CL05B104KB54PNC
Unique ID
gge92
Reuse Block

Group ID

Channel ID
$1I144
PCB Layer
TopLayer
Convert to PCB
yes

*
]
[
DESIGNATOR
C21
FOOTPRINT
C0402
PARTTYPE
CL05B104KB54PNC
DESCRIPTION
容值:100nF;精度:±10%;额定电压:50V;温度系数:X7R;
Component Kind
Standard
Footprint
C0402
Designator
C21
LCSC Part Name
100nF ±10% 50V
Supplier Part
C307331
Manufacturer
SAMSUNG(三星)
Manufacturer Part
CL05B104KB54PNC
Supplier Footprint
0402
JLCPCB Part Class
Basic Part
Datasheet
https://item.szlcsc.com/datasheet/CL05B104KB54PNC/291005.html
Supplier
LCSC
Add into BOM
yes
3D Model Title
C0402_L1.0-W0.5-H0.5
Value
100nF
Tolerance
±10%
Voltage Rating
50V
Temperature Coefficient
X7R
Name
100nF
Description
容值:100nF;精度:±10%;额定电压:50V;温度系数:X7R;
Device
CL05B104KB54PNC
Unique ID
gge9_3
Reuse Block

Group ID

Channel ID
$1I149
PCB Layer
TopLayer
Convert to PCB
yes

*
]
[
DESIGNATOR
C22
FOOTPRINT
C0402
PARTTYPE
CL05B104KB54PNC
DESCRIPTION
容值:100nF;精度:±10%;额定电压:50V;温度系数:X7R;
Component Kind
Standard
Footprint
C0402
Designator
C22
LCSC Part Name
100nF ±10% 50V
Supplier Part
C307331
Manufacturer
SAMSUNG(三星)
Manufacturer Part
CL05B104KB54PNC
Supplier Footprint
0402
JLCPCB Part Class
Basic Part
Datasheet
https://item.szlcsc.com/datasheet/CL05B104KB54PNC/291005.html
Supplier
LCSC
Add into BOM
yes
3D Model Title
C0402_L1.0-W0.5-H0.5
Value
100nF
Tolerance
±10%
Voltage Rating
50V
Temperature Coefficient
X7R
Name
100nF
Description
容值:100nF;精度:±10%;额定电压:50V;温度系数:X7R;
Device
CL05B104KB54PNC
Unique ID
gge9_4
Reuse Block

Group ID

Channel ID
$1I151
PCB Layer
TopLayer
Convert to PCB
yes

*
]
[
DESIGNATOR
D1
FOOTPRINT
LED-SMD_L1.6-W0.8-R-RD
PARTTYPE
KT-0603R
DESCRIPTION
灯头类型:1.6mmx0.8mm方形灯头;发光颜色:红色;正向压降(Vf):1.8V~2.4V;功率:40mW;正向电流:20mA;波长:615nm~630nm;二极管配置:独立二极管;透镜颜色:无色透明透镜;色温:-;发光强度:300mcd;发光角度:120°;载带方式:-;工作温度:-40℃~+85℃;
Component Kind
Standard
Name
KT-0603R
Device
KT-0603R
Designator
D1
Footprint
LED-SMD_L1.6-W0.8-R-RD
LCSC Part Name
0603 红灯 高亮
Supplier Part
C2286
Manufacturer
KENTO
Manufacturer Part
KT-0603R
Supplier Footprint
0603
JLCPCB Part Class
Basic Part
Datasheet
https://item.szlcsc.com/datasheet/KT-0603R/2659.html
Supplier
LCSC
Add into BOM
yes
3D Model Title
LED0603_L1.6-W0.8-H0.6
Lamp Holder Type
1.6mmx0.8mm方形灯头
Illumination Color
红色
Voltage - Forward(Vf)
1.8V~2.4V
Power(Watts)
40mW
Forward Current
20mA
Wavelength - Dominant
615nm~630nm
Peak Wavelength
645nm
Diode Configuration
独立二极管
Lens Color
无色透明透镜
Color Temperature
-
Luminous Intensity
300mcd
Viewing Angle
120°
Mounting Style
-
Operating Temperature
-40℃~+85℃
Description
灯头类型:1.6mmx0.8mm方形灯头;发光颜色:红色;正向压降(Vf):1.8V~2.4V;功率:40mW;正向电流:20mA;波长:615nm~630nm;二极管配置:独立二极管;透镜颜色:无色透明透镜;色温:-;发光强度:300mcd;发光角度:120°;载带方式:-;工作温度:-40℃~+85℃;
Unique ID
gge15_0
Reuse Block

Group ID

Channel ID
$1I67
PCB Layer
TopLayer
Convert to PCB
yes

*
]
[
DESIGNATOR
J1
FOOTPRINT
USB-C-SMD_TYPE-C-16PIN-2MD-073
PARTTYPE
TYPE-C 16PIN 2MD(073)
DESCRIPTION
连接器类型:Type-C;协议标准:-;公母:母;安装方式:卧贴;触点数量:16P;端口数量:1;额定电流 - 电源:3A;工作温度:-25℃~+85℃;
Component Kind
Standard
Footprint
USB-C-SMD_TYPE-C-16PIN-2MD-073
Designator
J1
LCSC Part Name
Type-C 母 卧贴
Supplier Part
C2765186
Manufacturer
SHOU HAN(首韩)
Manufacturer Part
TYPE-C 16PIN 2MD(073)
Supplier Footprint
SMD
JLCPCB Part Class
Extended Part
Datasheet
https://item.szlcsc.com/datasheet/TYPE-C%252016PIN%25202MD(073)/2901843.html
Supplier
LCSC
Add into BOM
yes
3D Model Title
USB-C-SMD_TYPE-C-6PIN-2MD-073
Connector Type
Type-C
Protocol Standard
-
Gender
母
Mounting Type
卧贴
Number of Contacts
16P
Number of Ports
1
Current Rating-Power
3A
Voltage Rating
5V
Connect-Disconnect Life
1万次
Supplementary Features
-
Center Height
-
Length
-
Detection color
黑色
Operating Temperature
-25℃~+85℃
Name
TYPE-C 16PIN 2MD(073)
Description
连接器类型:Type-C;协议标准:-;公母:母;安装方式:卧贴;触点数量:16P;端口数量:1;额定电流 - 电源:3A;工作温度:-25℃~+85℃;
Device
TYPE-C 16PIN 2MD(073)
Unique ID
gge37
Reuse Block

Group ID

Channel ID
$1I81
PCB Layer
TopLayer
Convert to PCB
yes

*
]
[
DESIGNATOR
J2
FOOTPRINT
CONN-TH_B8B-XH-AM-LF-SN
PARTTYPE
B8B-XH-AM(LF)(SN)
DESCRIPTION
插针结构:1x8P;间距:2.5mm;安装方式:直插;参考系列:XH;总PIN数:8P;排数:1;每排PIN数:8;行距:-;额定电流:3A;触头材质:黄铜;触头镀层:锡;工作温度:-25℃~+85℃;
Component Kind
Standard
Footprint
CONN-TH_B8B-XH-AM-LF-SN
Designator
J2
LCSC Part Name
1x8P 间距:2.5mm 直插 系列:XH
Supplier Part
C161875
Manufacturer
JST
Manufacturer Part
B8B-XH-AM(LF)(SN)
Supplier Footprint
插件,P=2.5mm
JLCPCB Part Class
Extended Part
Datasheet
https://item.szlcsc.com/datasheet/B8B-XH-AM(LF)(SN)/173256.html
Supplier
LCSC
Add into BOM
yes
3D Model Title
CONN-TH_B8B-XH-AM (LF)(SN)
Pins Structure
1x8P
Pitch
2.5mm
Mounting Type
直插
Reference Series
XH
Number of Pins
8P
Number of Rows
1
Number of PINs Per Row
8
Row Spacing
-
Current Rating
3A
Contact Material
黄铜
Contact Plating
锡
Operating Temperature
-25℃~+85℃
Voltage Rating
250V
Plastic Material
PA66
Flame Retardant Rating
UL94V-0
Supplementary Features
带柱；打K脚
Color
白色
Z-Height of the Board
7mm
X-Length of Bottom Edge on Board (Spacing Line)
22.4mm
Y-Width of Bottom Edge on Board
5.75mm
Name
B8B-XH-AM(LF)(SN)
Description
插针结构:1x8P;间距:2.5mm;安装方式:直插;参考系列:XH;总PIN数:8P;排数:1;每排PIN数:8;行距:-;额定电流:3A;触头材质:黄铜;触头镀层:锡;工作温度:-25℃~+85℃;
Device
B8B-XH-AM(LF)(SN)
Unique ID
gge33
Reuse Block

Group ID

Channel ID
$1I62
PCB Layer
TopLayer
Convert to PCB
yes

*
]
[
DESIGNATOR
J3
FOOTPRINT
CONN-TH_B2B-XH-A-LF-SN
PARTTYPE
B2B-XH-A(LF)(SN)
DESCRIPTION
插针结构:1x2P;间距:2.5mm;安装方式:直插;参考系列:XH;总PIN数:2P;排数:1;每排PIN数:2;行距:-;额定电流:3A;触头材质:黄铜;触头镀层:锡;工作温度:-25℃~+85℃;
Component Kind
Standard
Footprint
CONN-TH_B2B-XH-A-LF-SN
Designator
J3
LCSC Part Name
1x2P 间距:2.5mm 直插 系列:XH
Supplier Part
C158012
Manufacturer
JST
Manufacturer Part
B2B-XH-A(LF)(SN)
Supplier Footprint
插件,P=2.5mm
JLCPCB Part Class
Extended Part
Datasheet
https://item.szlcsc.com/datasheet/B2B-XH-A(LF)(SN)/169360.html
Supplier
LCSC
Add into BOM
yes
3D Model Title
XH2.5-2A
Pins Structure
1x2P
Pitch
2.5mm
Mounting Type
直插
Reference Series
XH
Number of Pins
2P
Number of Rows
1
Number of PINs Per Row
2
Row Spacing
-
Current Rating
3A
Contact Material
黄铜
Contact Plating
锡
Operating Temperature
-25℃~+85℃
Voltage Rating
250V
Plastic Material
PA66
Flame Retardant Rating
UL94V-0
Supplementary Features
打K脚
Color
白色
Z-Height of the Board
7mm
X-Length of Bottom Edge on Board (Spacing Line)
7.4mm
Y-Width of Bottom Edge on Board
5.75mm
Name
B2B-XH-A(LF)(SN)
Description
插针结构:1x2P;间距:2.5mm;安装方式:直插;参考系列:XH;总PIN数:2P;排数:1;每排PIN数:2;行距:-;额定电流:3A;触头材质:黄铜;触头镀层:锡;工作温度:-25℃~+85℃;
Device
B2B-XH-A(LF)(SN)
Unique ID
gge32_0
Reuse Block

Group ID

Channel ID
$1I156
PCB Layer
TopLayer
Convert to PCB
yes

*
]
[
DESIGNATOR
J4
FOOTPRINT
CONN-TH_3P-P2.50_A2501WV2-3P
PARTTYPE
B3B-XH-A(LF)(SN)
DESCRIPTION
插针结构:1x3P;间距:2.5mm;安装方式:直插;参考系列:XH;总PIN数:3P;排数:1;每排PIN数:3;行距:-;额定电流:3A;触头材质:黄铜;触头镀层:锡;工作温度:-25℃~+85℃;
Component Kind
Standard
Footprint
CONN-TH_3P-P2.50_A2501WV2-3P
Designator
J4
LCSC Part Name
1x3P 间距:2.5mm 直插 系列:XH
Supplier Part
C144394
Manufacturer
JST
Manufacturer Part
B3B-XH-A(LF)(SN)
Supplier Footprint
插件,P=2.5mm
JLCPCB Part Class
Extended Part
Datasheet
https://item.szlcsc.com/datasheet/B3B-XH-A(LF)(SN)/155726.html
Supplier
LCSC
Add into BOM
yes
3D Model Title
CONN-TH_3P-P2.50_A2501WV2-3P
Pins Structure
1x3P
Pitch
2.5mm
Mounting Type
直插
Reference Series
XH
Number of Pins
3P
Number of Rows
1
Number of PINs Per Row
3
Row Spacing
-
Current Rating
3A
Contact Material
黄铜
Contact Plating
锡
Operating Temperature
-25℃~+85℃
Voltage Rating
250V
Plastic Material
PA66
Flame Retardant Rating
UL94V-0
Supplementary Features
打K脚
Color
白色
Z-Height of the Board
7mm
X-Length of Bottom Edge on Board (Spacing Line)
9.9mm
Y-Width of Bottom Edge on Board
5.75mm
Name
B3B-XH-A(LF)(SN)
Description
插针结构:1x3P;间距:2.5mm;安装方式:直插;参考系列:XH;总PIN数:3P;排数:1;每排PIN数:3;行距:-;额定电流:3A;触头材质:黄铜;触头镀层:锡;工作温度:-25℃~+85℃;
Device
B3B-XH-A(LF)(SN)
Unique ID
gge46
Reuse Block

Group ID

Channel ID
$1I96
PCB Layer
TopLayer
Convert to PCB
yes

*
]
[
DESIGNATOR
J6
FOOTPRINT
CONN-TH_B4B-XH-A-LF-SN
PARTTYPE
B4B-XH-A(LF)(SN)
DESCRIPTION
插针结构:1x4P;间距:2.5mm;安装方式:直插;参考系列:XH;总PIN数:4P;排数:1;每排PIN数:4;行距:-;额定电流:3A;触头材质:黄铜;触头镀层:锡;工作温度:-25℃~+85℃;
Component Kind
Standard
Footprint
CONN-TH_B4B-XH-A-LF-SN
Designator
J6
LCSC Part Name
1x4P 间距:2.5mm 直插 系列:XH
Supplier Part
C144395
Manufacturer
JST
Manufacturer Part
B4B-XH-A(LF)(SN)
Supplier Footprint
插件,P=2.5mm
JLCPCB Part Class
Extended Part
Datasheet
https://item.szlcsc.com/datasheet/B4B-XH-A(LF)(SN)/155727.html
Supplier
LCSC
Add into BOM
yes
3D Model Title
XH2.5-4A
Pins Structure
1x4P
Pitch
2.5mm
Mounting Type
直插
Reference Series
XH
Number of Pins
4P
Number of Rows
1
Number of PINs Per Row
4
Row Spacing
-
Current Rating
3A
Contact Material
黄铜
Contact Plating
锡
Operating Temperature
-25℃~+85℃
Voltage Rating
250V
Plastic Material
PA66
Flame Retardant Rating
UL94V-0
Supplementary Features
打K脚
Color
白色
Z-Height of the Board
7mm
X-Length of Bottom Edge on Board (Spacing Line)
12.4mm
Y-Width of Bottom Edge on Board
5.75mm
Name
B4B-XH-A(LF)(SN)
Description
插针结构:1x4P;间距:2.5mm;安装方式:直插;参考系列:XH;总PIN数:4P;排数:1;每排PIN数:4;行距:-;额定电流:3A;触头材质:黄铜;触头镀层:锡;工作温度:-25℃~+85℃;
Device
B4B-XH-A(LF)(SN)
Unique ID
gge94
Reuse Block

Group ID

Channel ID
$1I155
PCB Layer
TopLayer
Convert to PCB
yes

*
]
[
DESIGNATOR
L1
FOOTPRINT
L0402
PARTTYPE
LQW15AN24NG00D
DESCRIPTION
电感值:24nH;精度:±2%;额定电流:280mA;饱和电流(Isat):-;类型:非屏蔽电感;
Component Kind
Standard
Footprint
L0402
Designator
L1
LCSC Part Name
24nH ±2%
Supplier Part
C167472
Manufacturer
muRata(村田)
Manufacturer Part
LQW15AN24NG00D
Supplier Footprint
0402
JLCPCB Part Class
Extended Part
Datasheet
https://item.szlcsc.com/datasheet/LQW15AN24NG00D/178855.html
Supplier
LCSC
Add into BOM
yes
3D Model Title
L0402_L1.0-W0.5-H0.5_BEAD
Value
24nH
Tolerance
±2%
Current Rating
280mA
Current - Saturation(Isat)
-
DC Resistance(DCR)
520mΩ
Type
非屏蔽电感
Ratings
-
Name
24nH
Description
电感值:24nH;精度:±2%;额定电流:280mA;饱和电流(Isat):-;类型:非屏蔽电感;
Device
LQW15AN24NG00D
Unique ID
gge59
Reuse Block

Group ID

Channel ID
$1I127
PCB Layer
TopLayer
Convert to PCB
yes

*
]
[
DESIGNATOR
L2
FOOTPRINT
L0603
PARTTYPE
BLM18PG121SN1D
DESCRIPTION
阻抗@频率:120Ω@100MHz;误差:±25%;直流电阻(DCR):50mΩ;
Component Kind
Standard
Footprint
L0603
Designator
L2
LCSC Part Name
单路 0603磁珠 阻抗120Ω@100MHz
Supplier Part
C14709
Manufacturer
muRata(村田)
Manufacturer Part
BLM18PG121SN1D
Supplier Footprint
0603
JLCPCB Part Class
Basic Part
Datasheet
https://item.szlcsc.com/datasheet/BLM18PG121SN1D/15379.html
Supplier
LCSC
Add into BOM
yes
3D Model Title
L0603_L1.6-W0.8-H0.5_BEAD
Impedance @ Frequency
120Ω@100MHz
Tolerance
±25%
DC Resistance(DCR)
50mΩ
Current Rating
2A
Number of Circuits
1
Operating Temperature
-55℃~+125℃
Name
BLM18PG121SN1D
Description
阻抗@频率:120Ω@100MHz;误差:±25%;直流电阻(DCR):50mΩ;
Device
BLM18PG121SN1D
Unique ID
gge89
Reuse Block

Group ID

Channel ID
$1I140
PCB Layer
TopLayer
Convert to PCB
yes

*
]
[
DESIGNATOR
L3
FOOTPRINT
IND-SMD_L4.4-W4.2
PARTTYPE
FXL0420-1R0-M
DESCRIPTION
电感值:1uH;精度:±20%;额定电流:6A;饱和电流(Isat):7A;类型:一体成型电感;
Component Kind
Standard
Footprint
IND-SMD_L4.4-W4.2
Designator
L3
LCSC Part Name
1uH ±20% 7A
Supplier Part
C167203
Manufacturer
cjiang(长江微电)
Manufacturer Part
FXL0420-1R0-M
Supplier Footprint
SMD,4.2x4.4mm
JLCPCB Part Class
Extended Part
Datasheet
https://atta.szlcsc.com/upload/public/pdf/source/20240426/3189EA8206330E2108542F9E34E540E7.pdf
Supplier
LCSC
Add into BOM
yes
3D Model Title
IND-SMD_L4.2-W4.4-H2.0
Value
1uH
Tolerance
±20%
Rated Current
6A
Saturation Current (Isat)
7A
DC Resistance (DCR)
27mΩ
Type
一体成型电感
Name
1uH
Description
电感值:1uH;精度:±20%;额定电流:6A;饱和电流(Isat):7A;类型:一体成型电感;
Device
FXL0420-1R0-M
Unique ID
gge97
Reuse Block

Group ID

Channel ID
$1I160
PCB Layer
TopLayer
Convert to PCB
yes

*
]
[
DESIGNATOR
R1
FOOTPRINT
R0402
PARTTYPE
0402WGF1002TCE
DESCRIPTION
电阻类型:厚膜电阻;阻值:10kΩ;精度:±1%;功率:62.5mW;工作电压:50V;温度系数:±100ppm/℃;
Component Kind
Standard
Footprint
R0402
Designator
R1
LCSC Part Name
10kΩ ±1% 62.5mW 厚膜电阻
Supplier Part
C25744
Manufacturer
UNI-ROYAL(厚声)
Manufacturer Part
0402WGF1002TCE
Supplier Footprint
0402
JLCPCB Part Class
Basic Part
Datasheet
https://item.szlcsc.com/datasheet/0402WGF1002TCE/26487.html
Supplier
LCSC
Add into BOM
yes
3D Model Title
R0402_L1.0-W0.5-H0.4
Type
厚膜电阻
Value
10kΩ
Tolerance
±1%
Power(Watts)
62.5mW
Voltage-Supply(Max)
50V
Temperature Coefficient
±100ppm/℃
Operating Temperature
-55℃~+155℃
Name
10kΩ
Description
电阻类型:厚膜电阻;阻值:10kΩ;精度:±1%;功率:62.5mW;工作电压:50V;温度系数:±100ppm/℃;
Device
0402WGF1002TCE
Unique ID
gge12
Reuse Block

Group ID

Channel ID
$1I108
PCB Layer
TopLayer
Convert to PCB
yes

*
]
[
DESIGNATOR
R2
FOOTPRINT
R0402
PARTTYPE
0402WGF1001TCE
DESCRIPTION
电阻类型:厚膜电阻;阻值:1kΩ;精度:±1%;功率:62.5mW;工作电压:50V;温度系数:±100ppm/℃;
Component Kind
Standard
Footprint
R0402
Designator
R2
LCSC Part Name
1kΩ ±1% 62.5mW 厚膜电阻
Supplier Part
C11702
Manufacturer
UNI-ROYAL(厚声)
Manufacturer Part
0402WGF1001TCE
Supplier Footprint
0402
JLCPCB Part Class
Basic Part
Datasheet
https://item.szlcsc.com/datasheet/0402WGF1001TCE/12256.html
Supplier
LCSC
Add into BOM
yes
3D Model Title
R0402_L1.0-W0.5-H0.4
Type
厚膜电阻
Value
1kΩ
Tolerance
±1%
Power(Watts)
62.5mW
Voltage-Supply(Max)
50V
Temperature Coefficient
±100ppm/℃
Operating Temperature
-55℃~+155℃
Name
1kΩ
Description
电阻类型:厚膜电阻;阻值:1kΩ;精度:±1%;功率:62.5mW;工作电压:50V;温度系数:±100ppm/℃;
Device
0402WGF1001TCE
Unique ID
gge96
Reuse Block

Group ID

Channel ID
$1I159
PCB Layer
TopLayer
Convert to PCB
yes

*
]
[
DESIGNATOR
R3
FOOTPRINT
R0402
PARTTYPE
0402WGF4701TCE
DESCRIPTION
电阻类型:厚膜电阻;阻值:4.7kΩ;精度:±1%;功率:62.5mW;工作电压:50V;温度系数:±100ppm/℃;
Component Kind
Standard
Footprint
R0402
Designator
R3
LCSC Part Name
4.7kΩ ±1% 62.5mW 厚膜电阻
Supplier Part
C25900
Manufacturer
UNI-ROYAL(厚声)
Manufacturer Part
0402WGF4701TCE
Supplier Footprint
0402
JLCPCB Part Class
Basic Part
Datasheet
https://item.szlcsc.com/datasheet/0402WGF4701TCE/26643.html
Supplier
LCSC
Add into BOM
yes
3D Model Title
R0402_L1.0-W0.5-H0.4
Type
厚膜电阻
Value
4.7kΩ
Tolerance
±1%
Power(Watts)
62.5mW
Voltage-Supply(Max)
50V
Temperature Coefficient
±100ppm/℃
Operating Temperature
-55℃~+155℃
Name
4.7kΩ
Description
电阻类型:厚膜电阻;阻值:4.7kΩ;精度:±1%;功率:62.5mW;工作电压:50V;温度系数:±100ppm/℃;
Device
0402WGF4701TCE
Unique ID
gge16
Reuse Block

Group ID

Channel ID
$1I110
PCB Layer
TopLayer
Convert to PCB
yes

*
]
[
DESIGNATOR
R4
FOOTPRINT
R0402
PARTTYPE
0402WGF4701TCE
DESCRIPTION
电阻类型:厚膜电阻;阻值:4.7kΩ;精度:±1%;功率:62.5mW;工作电压:50V;温度系数:±100ppm/℃;
Component Kind
Standard
Footprint
R0402
Designator
R4
LCSC Part Name
4.7kΩ ±1% 62.5mW 厚膜电阻
Supplier Part
C25900
Manufacturer
UNI-ROYAL(厚声)
Manufacturer Part
0402WGF4701TCE
Supplier Footprint
0402
JLCPCB Part Class
Basic Part
Datasheet
https://item.szlcsc.com/datasheet/0402WGF4701TCE/26643.html
Supplier
LCSC
Add into BOM
yes
3D Model Title
R0402_L1.0-W0.5-H0.4
Type
厚膜电阻
Value
4.7kΩ
Tolerance
±1%
Power(Watts)
62.5mW
Voltage-Supply(Max)
50V
Temperature Coefficient
±100ppm/℃
Operating Temperature
-55℃~+155℃
Name
4.7kΩ
Description
电阻类型:厚膜电阻;阻值:4.7kΩ;精度:±1%;功率:62.5mW;工作电压:50V;温度系数:±100ppm/℃;
Device
0402WGF4701TCE
Unique ID
gge17
Reuse Block

Group ID

Channel ID
$1I111
PCB Layer
TopLayer
Convert to PCB
yes

*
]
[
DESIGNATOR
R5
FOOTPRINT
R0402
PARTTYPE
0402WGF1002TCE
DESCRIPTION
电阻类型:厚膜电阻;阻值:10kΩ;精度:±1%;功率:62.5mW;工作电压:50V;温度系数:±100ppm/℃;
Component Kind
Standard
Footprint
R0402
Designator
R5
LCSC Part Name
10kΩ ±1% 62.5mW 厚膜电阻
Supplier Part
C25744
Manufacturer
UNI-ROYAL(厚声)
Manufacturer Part
0402WGF1002TCE
Supplier Footprint
0402
JLCPCB Part Class
Basic Part
Datasheet
https://item.szlcsc.com/datasheet/0402WGF1002TCE/26487.html
Supplier
LCSC
Add into BOM
yes
3D Model Title
R0402_L1.0-W0.5-H0.4
Type
厚膜电阻
Value
10kΩ
Tolerance
±1%
Power(Watts)
62.5mW
Voltage-Supply(Max)
50V
Temperature Coefficient
±100ppm/℃
Operating Temperature
-55℃~+155℃
Name
10kΩ
Description
电阻类型:厚膜电阻;阻值:10kΩ;精度:±1%;功率:62.5mW;工作电压:50V;温度系数:±100ppm/℃;
Device
0402WGF1002TCE
Unique ID
gge18
Reuse Block

Group ID

Channel ID
$1I114
PCB Layer
TopLayer
Convert to PCB
yes

*
]
[
DESIGNATOR
R6
FOOTPRINT
R0402
PARTTYPE
0402WGF5101TCE
DESCRIPTION
电阻类型:厚膜电阻;阻值:5.1kΩ;精度:±1%;功率:62.5mW;工作电压:50V;温度系数:±100ppm/℃;
Component Kind
Standard
Footprint
R0402
Designator
R6
LCSC Part Name
5.1kΩ ±1% 62.5mW 厚膜电阻
Supplier Part
C25905
Manufacturer
UNI-ROYAL(厚声)
Manufacturer Part
0402WGF5101TCE
Supplier Footprint
0402
JLCPCB Part Class
Basic Part
Datasheet
https://item.szlcsc.com/datasheet/0402WGF5101TCE/26648.html
Supplier
LCSC
Add into BOM
yes
3D Model Title
R0402_L1.0-W0.5-H0.4
Type
厚膜电阻
Value
5.1kΩ
Tolerance
±1%
Power(Watts)
62.5mW
Voltage-Supply(Max)
50V
Temperature Coefficient
±100ppm/℃
Operating Temperature
-55℃~+155℃
Name
5.1kΩ
Description
电阻类型:厚膜电阻;阻值:5.1kΩ;精度:±1%;功率:62.5mW;工作电压:50V;温度系数:±100ppm/℃;
Device
0402WGF5101TCE
Unique ID
gge30
Reuse Block

Group ID

Channel ID
$1I55
PCB Layer
TopLayer
Convert to PCB
yes

*
]
[
DESIGNATOR
R7
FOOTPRINT
R0402
PARTTYPE
0402WGF5101TCE
DESCRIPTION
电阻类型:厚膜电阻;阻值:5.1kΩ;精度:±1%;功率:62.5mW;工作电压:50V;温度系数:±100ppm/℃;
Component Kind
Standard
Footprint
R0402
Designator
R7
LCSC Part Name
5.1kΩ ±1% 62.5mW 厚膜电阻
Supplier Part
C25905
Manufacturer
UNI-ROYAL(厚声)
Manufacturer Part
0402WGF5101TCE
Supplier Footprint
0402
JLCPCB Part Class
Basic Part
Datasheet
https://item.szlcsc.com/datasheet/0402WGF5101TCE/26648.html
Supplier
LCSC
Add into BOM
yes
3D Model Title
R0402_L1.0-W0.5-H0.4
Type
厚膜电阻
Value
5.1kΩ
Tolerance
±1%
Power(Watts)
62.5mW
Voltage-Supply(Max)
50V
Temperature Coefficient
±100ppm/℃
Operating Temperature
-55℃~+155℃
Name
5.1kΩ
Description
电阻类型:厚膜电阻;阻值:5.1kΩ;精度:±1%;功率:62.5mW;工作电压:50V;温度系数:±100ppm/℃;
Device
0402WGF5101TCE
Unique ID
gge29
Reuse Block

Group ID

Channel ID
$1I54
PCB Layer
TopLayer
Convert to PCB
yes

*
]
[
DESIGNATOR
R9
FOOTPRINT
R0402
PARTTYPE
0402WGF220JTCE
DESCRIPTION
电阻类型:厚膜电阻;阻值:22Ω;精度:±1%;功率:62.5mW;最大工作电压:50V;温度系数:±100ppm/℃;
Component Kind
Standard
Footprint
R0402
Designator
R9
LCSC Part Name
22Ω ±1% 62.5mW 厚膜电阻
Supplier Part
C25092
Manufacturer
UNI-ROYAL(厚声)
Manufacturer Part
0402WGF220JTCE
Supplier Footprint
0402
JLCPCB Part Class
Basic Part
Datasheet
https://atta.szlcsc.com/upload/public/pdf/source/20200306/C422600_1E6D84923E4A46A82E41ADD87F860B5C.pdf
Supplier
LCSC
Add into BOM
yes
3D Model Title
R0402_L1.0-W0.5-H0.4
Type
厚膜电阻
Value
22Ω
Tolerance
±1%
Power(Watts)
62.5mW
Overload Voltage (Max)
50V
Temperature Coefficient
±100ppm/℃
Operating Temperature Range
-55℃~+155℃
Name
22Ω
Description
电阻类型:厚膜电阻;阻值:22Ω;精度:±1%;功率:62.5mW;最大工作电压:50V;温度系数:±100ppm/℃;
Device
0402WGF220JTCE
Unique ID
gge39
Reuse Block

Group ID

Channel ID
$1I112
PCB Layer
TopLayer
Convert to PCB
yes

*
]
[
DESIGNATOR
R10
FOOTPRINT
R0402
PARTTYPE
0402WGF220JTCE
DESCRIPTION
电阻类型:厚膜电阻;阻值:22Ω;精度:±1%;功率:62.5mW;最大工作电压:50V;温度系数:±100ppm/℃;
Component Kind
Standard
Footprint
R0402
Designator
R10
LCSC Part Name
22Ω ±1% 62.5mW 厚膜电阻
Supplier Part
C25092
Manufacturer
UNI-ROYAL(厚声)
Manufacturer Part
0402WGF220JTCE
Supplier Footprint
0402
JLCPCB Part Class
Basic Part
Datasheet
https://atta.szlcsc.com/upload/public/pdf/source/20200306/C422600_1E6D84923E4A46A82E41ADD87F860B5C.pdf
Supplier
LCSC
Add into BOM
yes
3D Model Title
R0402_L1.0-W0.5-H0.4
Type
厚膜电阻
Value
22Ω
Tolerance
±1%
Power(Watts)
62.5mW
Overload Voltage (Max)
50V
Temperature Coefficient
±100ppm/℃
Operating Temperature Range
-55℃~+155℃
Name
22Ω
Description
电阻类型:厚膜电阻;阻值:22Ω;精度:±1%;功率:62.5mW;最大工作电压:50V;温度系数:±100ppm/℃;
Device
0402WGF220JTCE
Unique ID
gge40
Reuse Block

Group ID

Channel ID
$1I113
PCB Layer
TopLayer
Convert to PCB
yes

*
]
[
DESIGNATOR
R11
FOOTPRINT
R0402
PARTTYPE
0402WGF1002TCE
DESCRIPTION
电阻类型:厚膜电阻;阻值:10kΩ;精度:±1%;功率:62.5mW;工作电压:50V;温度系数:±100ppm/℃;
Component Kind
Standard
Footprint
R0402
Designator
R11
LCSC Part Name
10kΩ ±1% 62.5mW 厚膜电阻
Supplier Part
C25744
Manufacturer
UNI-ROYAL(厚声)
Manufacturer Part
0402WGF1002TCE
Supplier Footprint
0402
JLCPCB Part Class
Basic Part
Datasheet
https://item.szlcsc.com/datasheet/0402WGF1002TCE/26487.html
Supplier
LCSC
Add into BOM
yes
3D Model Title
R0402_L1.0-W0.5-H0.4
Type
厚膜电阻
Value
10kΩ
Tolerance
±1%
Power(Watts)
62.5mW
Voltage-Supply(Max)
50V
Temperature Coefficient
±100ppm/℃
Operating Temperature
-55℃~+155℃
Name
10kΩ
Description
电阻类型:厚膜电阻;阻值:10kΩ;精度:±1%;功率:62.5mW;工作电压:50V;温度系数:±100ppm/℃;
Device
0402WGF1002TCE
Unique ID
gge12_0
Reuse Block

Group ID

Channel ID
$1I119
PCB Layer
TopLayer
Convert to PCB
yes

*
]
[
DESIGNATOR
R12
FOOTPRINT
R0402
PARTTYPE
0402WGF1002TCE
DESCRIPTION
电阻类型:厚膜电阻;阻值:10kΩ;精度:±1%;功率:62.5mW;工作电压:50V;温度系数:±100ppm/℃;
Component Kind
Standard
Footprint
R0402
Designator
R12
LCSC Part Name
10kΩ ±1% 62.5mW 厚膜电阻
Supplier Part
C25744
Manufacturer
UNI-ROYAL(厚声)
Manufacturer Part
0402WGF1002TCE
Supplier Footprint
0402
JLCPCB Part Class
Basic Part
Datasheet
https://item.szlcsc.com/datasheet/0402WGF1002TCE/26487.html
Supplier
LCSC
Add into BOM
yes
3D Model Title
R0402_L1.0-W0.5-H0.4
Type
厚膜电阻
Value
10kΩ
Tolerance
±1%
Power(Watts)
62.5mW
Voltage-Supply(Max)
50V
Temperature Coefficient
±100ppm/℃
Operating Temperature
-55℃~+155℃
Name
10kΩ
Description
电阻类型:厚膜电阻;阻值:10kΩ;精度:±1%;功率:62.5mW;工作电压:50V;温度系数:±100ppm/℃;
Device
0402WGF1002TCE
Unique ID
gge12_1
Reuse Block

Group ID

Channel ID
$1I120
PCB Layer
TopLayer
Convert to PCB
yes

*
]
[
DESIGNATOR
RESET
FOOTPRINT
SW-SMD_L3.9-W3.0-P4.45
PARTTYPE
TS-1088-AR02016
DESCRIPTION
电路结构:单刀单掷;按钮形状:圆形按钮;作用力:1.6N;安装方式:立贴;开关长度:3.9mm;开关宽度:3mm;开关高度:2mm;带支架:不带支架;触点电流:50mA;额定电压:12V;带灯:-;工作寿命:10万次;
Component Kind
Standard
Footprint
SW-SMD_L3.9-W3.0-P4.45
Designator
RESET
LCSC Part Name
3.9*3*2mm 立贴 轻触开关
Supplier Part
C720477
Manufacturer
XUNPU(讯普)
Manufacturer Part
TS-1088-AR02016
Supplier Footprint
SMD,4x3mm
JLCPCB Part Class
Basic Part
Datasheet
https://item.szlcsc.com/datasheet/TS-1088-AR02016/763484.html
Supplier
LCSC
Add into BOM
yes
3D Model Title
SW-SMD_L3.9-W2.9-H2.0-LS4.8
Circuit
单刀单掷
Actuator Style
圆形按钮
Operating Force
1.6N
Mounting Type
立贴
Length
3.9mm
Width
3mm
Switch Height
2mm
with Bracket
不带支架
Contact Current
50mA
Voltage Rating
12V
Actuator/Cap Color
黑色
With Lamp
-
IP Rating
-
Termination Style
SMD接片
Life
10万次
Operating Temperature
-30℃~+80℃
Name
TS-1088-AR02016
Description
电路结构:单刀单掷;按钮形状:圆形按钮;作用力:1.6N;安装方式:立贴;开关长度:3.9mm;开关宽度:3mm;开关高度:2mm;带支架:不带支架;触点电流:50mA;额定电压:12V;带灯:-;工作寿命:10万次;
Device
TS-1088-AR02016
Unique ID
gge19
Reuse Block

Group ID

Channel ID
$1I115
PCB Layer
TopLayer
Convert to PCB
yes

*
]
[
DESIGNATOR
SPK1
FOOTPRINT
BUZ-SMD_4P-L13.0-W13.0-P11.4-BL
PARTTYPE
FS-1340
DESCRIPTION
阻抗:8Ω;谐振频率:850Hz;失真(THD):5%;额定功率:700mW;声压(SPL):88dB;
Component Kind
Standard
Footprint
BUZ-SMD_4P-L13.0-W13.0-P11.4-BL
Designator
SPK1
LCSC Part Name
喇叭13*13MM-4.0H 8Ω0.5W 贴片
Supplier Part
C482342
Manufacturer
FUET(福声科技)
Manufacturer Part
FS-1340
Supplier Footprint
-
JLCPCB Part Class
Extended Part
Datasheet
https://item.szlcsc.com/datasheet/FS-1340/490268.html
Supplier
LCSC
Add into BOM
yes
3D Model Title
BUZ-SMD_4P-L13.0-W13.0-P11.4-BL
Frequency Range
850Hz~20kHz
Impedance
8Ω
Resonant Frequency
850Hz
Total Harmonic Distortion(THD)
5%
Rated Power
700mW
Sound Pressure Level(SPL)
88dB
Length
13mm
Width
13mm
Height
4mm
Operating Temperature
-40℃~+85℃
Mounting Type
贴片
Name
FS-1340
Description
阻抗:8Ω;谐振频率:850Hz;失真(THD):5%;额定功率:700mW;声压(SPL):88dB;
Device
FS-1340
Unique ID
gge95
Reuse Block

Group ID

Channel ID
$1I157
PCB Layer
TopLayer
Convert to PCB
yes

*
]
[
DESIGNATOR
U1
FOOTPRINT
QFN-56_L7.0-W7.0-P0.40-BL-EP5.7
PARTTYPE
ESP32-S3FH4R2
DESCRIPTION
核心芯片:LX7芯片;频率:2.4GHz;天线形式:-;发射功率:21dBm;接收灵敏度:-104.5dBm;
Component Kind
Standard
Footprint
QFN-56_L7.0-W7.0-P0.40-BL-EP5.7
Designator
U1
LCSC Part Name
不带固件 Xtensa 32位Lx7双核微处理器，2.4 GHz Wi-Fi和Bluetooth 5(LE)，45个GPIO管脚
Supplier Part
C3013940
Manufacturer
ESPRESSIF(乐鑫)
Manufacturer Part
ESP32-S3FH4R2
Supplier Footprint
QFN-56(7x7)
JLCPCB Part Class
Extended Part
Datasheet
https://item.szlcsc.com/datasheet/ESP32-S3FH4R2/3522410.html
Supplier
LCSC
Add into BOM
yes
Utilized IC / Part
LX7芯片
Wireless Standard
Bluetooth5.0
Interface Type
SDIO；JTAG；UART；SPI；I2C
Value
2.4GHz
Antenna Type
-
Output Power
21dBm
Voltage - Supply
3V~3.6V
Receive  Current
88mA
Send  Current
340mA
Sensitivity
-104.5dBm
Operating Temperature
-40℃~+85℃
Name
2.4GHz
Description
核心芯片:LX7芯片;频率:2.4GHz;天线形式:-;发射功率:21dBm;接收灵敏度:-104.5dBm;
Device
ESP32-S3FH4R2
Unique ID
gge90
3D Model Title
undefined
Reuse Block

Group ID

Channel ID
$1I97
PCB Layer
TopLayer
Convert to PCB
yes

*
]
[
DESIGNATOR
U2
FOOTPRINT
SOT-89_L4.5-W2.5-P1.50-LS4.2-BR
PARTTYPE
ME6211A33PG-N
DESCRIPTION
输出极性:正极;工作电压:6V;输出电压:3.3V;输出电流:500mA;电源纹波抑制比(PSRR):70dB@(1kHz);输出类型:固定;
Component Kind
Standard
Footprint
SOT-89_L4.5-W2.5-P1.50-LS4.2-BR
Designator
U2
LCSC Part Name
3.3V 500mA 6V
Supplier Part
C236673
Manufacturer
MICRONE(南京微盟)
Manufacturer Part
ME6211A33PG-N
Supplier Footprint
SOT-89
JLCPCB Part Class
Extended Part
Datasheet
https://item.szlcsc.com/datasheet/ME6211A33PG-N/236113.html
Supplier
LCSC
Add into BOM
yes
3D Model Title
SOT-89-3_L4.3-W2.5-H1.6-LS4.1-P1.50
Output Configuration
正极
Voltage - Supply
6V
Output Voltage
3.3V
Output Current
500mA
Power Supply Rejection Ratio (PSRR)
70dB@(1kHz)
Voltage Dropout
120mV@(100mA)
standby current
30uA
Noise
50uVrms
Features
使能控制；短路保护；过流保护
Operating Temperature
-40℃~+150℃@(Ta)
Output Type
固定
Number of Outputs
1
Name
ME6211A33PG-N
Description
输出极性:正极;工作电压:6V;输出电压:3.3V;输出电流:500mA;电源纹波抑制比(PSRR):70dB@(1kHz);输出类型:固定;
Device
ME6211A33PG-N
Unique ID
gge1
Reuse Block

Group ID

Channel ID
$1I4
PCB Layer
TopLayer
Convert to PCB
yes

*
]
[
DESIGNATOR
U3
FOOTPRINT
TQFN-16_L3.0-W3.0-P0.50-BL-EP1.5
PARTTYPE
MAX98357AETE+T
DESCRIPTION
功放类型:D类功放;扬声器通道数:-;输出功率:3.2W×1@4Ω;静态电流(Iq):2.4mA;
Component Kind
Standard
Footprint
TQFN-16_L3.0-W3.0-P0.50-BL-EP1.5
Designator
U3
LCSC Part Name
微型、低成本、PCM 类 D 级放大器具有 AB 级性能
Supplier Part
C910544
Manufacturer
ADI(亚德诺)/MAXIM(美信)
Manufacturer Part
MAX98357AETE+T
Supplier Footprint
TQFN-16-EP(3x3)
JLCPCB Part Class
Extended Part
Datasheet
https://item.szlcsc.com/datasheet/MAX98357AETE%252BT/978950.html
Supplier
LCSC
Add into BOM
yes
3D Model Title
TQFN-16_L3.0-W3.0-P0.50-BL-EP1.5
Class
D类功放
Speaker Channels
-
Output Power
3.2W×1@4Ω
Voltage - Supply
2.5V~5.5V
Total Harmonic Distortion + Noise (THD+N)
-
Quiescent Current
2.4mA
Operating Temperature
-40℃~+85℃
Power Supply Rejection Ratio (PSRR)
77dB
Efficiency
92%
Name
MAX98357AETE+T
Description
功放类型:D类功放;扬声器通道数:-;输出功率:3.2W×1@4Ω;静态电流(Iq):2.4mA;
Device
MAX98357AETE+T
Unique ID
gge23
Reuse Block

Group ID

Channel ID
$1I35
PCB Layer
TopLayer
Convert to PCB
yes

*
]
[
DESIGNATOR
U4
FOOTPRINT
ESOP-8_L4.9-W3.9-P1.27-LS6.0-BL-EP
PARTTYPE
IP5306
DESCRIPTION
工作电压:4.65V~5.5V;最大充电电流:2.1A;电池类型:锂电池;电池节数:1;
Component Kind
Standard
Footprint
ESOP-8_L4.9-W3.9-P1.27-LS6.0-BL-EP
Designator
U4
LCSC Part Name
集成2.1A充电器和2.1A放电器的移动电源系统级芯片
Supplier Part
C181692
Manufacturer
INJOINIC(英集芯)
Manufacturer Part
IP5306
Supplier Footprint
ESOP-8
JLCPCB Part Class
Extended Part
Datasheet
https://item.szlcsc.com/datasheet/IP5306/193089.html
Supplier
LCSC
Add into BOM
yes
3D Model Title
ESOP-8_L4.9-W3.9-H1.6-LS6.0-P1.27
The Chip Type
充电芯片；保护芯片
Voltage - Supply
4.65V~5.5V
Charge Current - Max
2.1A
Charging Saturation Voltage
4.2V
End-Off Voltage
3V
Type of Battery
锂电池
Number of Cells
1
Operating Temperature
0℃~+70℃
Battery Temperature Detection
不支持
0V Battery Charge
不支持
Supply Current (Iq)
100uA
Balance Current
-
Interface
I2C
Features
过流保护；恒流充电；自动再充电；充电终止；过压保护；欠压锁定；过放保护；涓流充电；短路保护
Name
IP5306
Description
工作电压:4.65V~5.5V;最大充电电流:2.1A;电池类型:锂电池;电池节数:1;
Device
IP5306
Unique ID
gge93
Reuse Block

Group ID

Channel ID
$1I153
PCB Layer
TopLayer
Convert to PCB
yes

*
]
[
DESIGNATOR
U5
FOOTPRINT
LGA-16_L3.0-W3.0-P0.50-TL
PARTTYPE
LIS3DHTR
DESCRIPTION
传感器类型:加速度计;接口类型:I2C；SPI;
Component Kind
Standard
Footprint
LGA-16_L3.0-W3.0-P0.50-TL
Designator
U5
LCSC Part Name
MEMS数字输出运动传感器：超低功耗、高性能三轴加速度计
Supplier Part
C15134
Manufacturer
ST(意法半导体)
Manufacturer Part
LIS3DHTR
Supplier Footprint
LGA-16(3x3)
JLCPCB Part Class
Extended Part
Datasheet
https://item.szlcsc.com/datasheet/LIS3DHTR/15808.html
Supplier
LCSC
Add into BOM
yes
3D Model Title
LGA-16_L3.0-W3.0-P0.50-TL
Accelerometer Sensing Axis
X,Y,Z
Acceleration Measurement Range (MAX)
±16g
Gyroscope Sensing Axis
-
Gyroscope Measurement Range (MAX)
-
Sensor Type
加速度计
Output Bits
16bit
Interface
I2C；SPI
Voltage - Supply
1.71V~3.6V
Cache Size
-
Standby Current
500nA
Operating Temperature
-40℃~+85℃
Features
运动事件检测
Name
LIS3DHTR
Description
传感器类型:加速度计;接口类型:I2C；SPI;
Device
LIS3DHTR
Unique ID
gge4
Reuse Block

Group ID

Channel ID
$1I8
PCB Layer
TopLayer
Convert to PCB
yes

*
]
[
DESIGNATOR
X1
FOOTPRINT
CRYSTAL-SMD_4P-L2.5-W2.0-BL
PARTTYPE
TXM40M0004252HBCEO00T
DESCRIPTION
晶振类型:贴片晶振;频率:40MHz;常温频差:±10ppm;负载电容:15pF;频率稳定度:±30ppm;
Component Kind
Standard
Footprint
CRYSTAL-SMD_4P-L2.5-W2.0-BL
Designator
X1
LCSC Part Name
40MHz ±10ppm 15pF
Supplier Part
C284176
Manufacturer
YJX(雅晶鑫)
Manufacturer Part
TXM40M0004252HBCEO00T
Supplier Footprint
SMD2520-4P
JLCPCB Part Class
Extended Part
Datasheet
https://item.szlcsc.com/datasheet/TXM40M0004252HBCEO00T/270225.html
Supplier
LCSC
Add into BOM
yes
3D Model Title
CRYSTAL-SMD_4P-L2.5-W2.0-BL
Type
贴片晶振
Value
40MHz
Normal temperature Frequency Tolerance
±10ppm
Load Capacitance
15pF
Frequency Stability
±30ppm
Equivalent Series Resistance(ESR)
25Ω
Operating Temperature
-40℃~+85℃
Name
40MHz
Description
晶振类型:贴片晶振;频率:40MHz;常温频差:±10ppm;负载电容:15pF;频率稳定度:±30ppm;
Device
TXM40M0004252HBCEO00T
Unique ID
gge91
Reuse Block

Group ID

Channel ID
$1I131
PCB Layer
TopLayer
Convert to PCB
yes

*
]
[
DESIGNATOR
R8
FOOTPRINT
R0603
PARTTYPE
0603WAF0000T5E
DESCRIPTION
电阻类型:厚膜电阻;阻值:0Ω;精度:±1%;功率:100mW;工作电压:75V;温度系数:-;
Component Kind
Standard
Footprint
R0603
Designator
R8
LCSC Part Name
0Ω ±1% 100mW 厚膜电阻
Supplier Part
C21189
Manufacturer
UNI-ROYAL(厚声)
Manufacturer Part
0603WAF0000T5E
Supplier Footprint
0603
JLCPCB Part Class
Basic Part
Datasheet
https://item.szlcsc.com/datasheet/0603WAF0000T5E/21903.html
Supplier
LCSC
Add into BOM
yes
3D Model Title
R0603
Type
厚膜电阻
Value
0Ω
Tolerance
±1%
Power(Watts)
100mW
Voltage-Supply(Max)
75V
Temperature Coefficient
-
Operating Temperature
-55℃~+155℃
Name
0Ω
Description
电阻类型:厚膜电阻;阻值:0Ω;精度:±1%;功率:100mW;工作电压:75V;温度系数:-;
Device
0603WAF0000T5E
Unique ID
gge101
Reuse Block

Group ID

Channel ID
$1I168
PCB Layer
TopLayer
Convert to PCB
yes

*
]
[
DESIGNATOR
R13
FOOTPRINT
R0402
PARTTYPE
0402WGF4702TCE
DESCRIPTION
电阻类型:厚膜电阻;阻值:47kΩ;精度:±1%;功率:62.5mW;工作电压:50V;温度系数:±100ppm/℃;
Component Kind
Standard
Footprint
R0402
Designator
R13
LCSC Part Name
47kΩ ±1% 62.5mW 厚膜电阻
Supplier Part
C25792
Manufacturer
UNI-ROYAL(厚声)
Manufacturer Part
0402WGF4702TCE
Supplier Footprint
0402
JLCPCB Part Class
Basic Part
Datasheet
https://item.szlcsc.com/datasheet/0402WGF4702TCE/26535.html
Supplier
LCSC
Add into BOM
yes
3D Model Title
R0402_L1.0-W0.5-H0.4
Type
厚膜电阻
Value
47kΩ
Tolerance
±1%
Power(Watts)
62.5mW
Voltage-Supply(Max)
50V
Temperature Coefficient
±100ppm/℃
Operating Temperature
-55℃~+155℃
Name
47kΩ
Description
电阻类型:厚膜电阻;阻值:47kΩ;精度:±1%;功率:62.5mW;工作电压:50V;温度系数:±100ppm/℃;
Device
0402WGF4702TCE
Unique ID
gge102
Reuse Block

Group ID

Channel ID
$1I169
PCB Layer
TopLayer
Convert to PCB
yes

*
]
[
DESIGNATOR
C23
FOOTPRINT
C0603
PARTTYPE
CL10A106KP8NNNC
DESCRIPTION
容值:10uF;精度:±10%;额定电压:10V;温度系数:X5R;
Component Kind
Standard
Footprint
C0603
Designator
C23
LCSC Part Name
10uF ±10% 10V
Supplier Part
C19702
Manufacturer
SAMSUNG(三星)
Manufacturer Part
CL10A106KP8NNNC
Supplier Footprint
0603
JLCPCB Part Class
Basic Part
Datasheet
https://item.szlcsc.com/datasheet/CL10A106KP8NNNC/20411.html
Supplier
LCSC
Add into BOM
yes
3D Model Title
C0603_L1.6-W0.8-H0.8
Value
10uF
Tolerance
±10%
Voltage Rating
10V
Temperature Coefficient
X5R
Name
10uF
Description
容值:10uF;精度:±10%;额定电压:10V;温度系数:X5R;
Device
CL10A106KP8NNNC
Unique ID
gge107
Reuse Block

Group ID

Channel ID
$1I178
PCB Layer
TopLayer
Convert to PCB
yes

*
]
[
DESIGNATOR
C25
FOOTPRINT
C0603
PARTTYPE
CL10A106KP8NNNC
DESCRIPTION
容值:10uF;精度:±10%;额定电压:10V;温度系数:X5R;
Component Kind
Standard
Footprint
C0603
Designator
C25
LCSC Part Name
10uF ±10% 10V
Supplier Part
C19702
Manufacturer
SAMSUNG(三星)
Manufacturer Part
CL10A106KP8NNNC
Supplier Footprint
0603
JLCPCB Part Class
Basic Part
Datasheet
https://item.szlcsc.com/datasheet/CL10A106KP8NNNC/20411.html
Supplier
LCSC
Add into BOM
yes
3D Model Title
C0603_L1.6-W0.8-H0.8
Value
10uF
Tolerance
±10%
Voltage Rating
10V
Temperature Coefficient
X5R
Name
10uF
Description
容值:10uF;精度:±10%;额定电压:10V;温度系数:X5R;
Device
CL10A106KP8NNNC
Unique ID
gge105
Reuse Block

Group ID

Channel ID
$1I176
PCB Layer
TopLayer
Convert to PCB
yes

*
]
[
DESIGNATOR
R14
FOOTPRINT
R0402
PARTTYPE
0402WGF1002TCE
DESCRIPTION
电阻类型:厚膜电阻;阻值:10kΩ;精度:±1%;功率:62.5mW;工作电压:50V;温度系数:±100ppm/℃;
Component Kind
Standard
Footprint
R0402
Designator
R14
LCSC Part Name
10kΩ ±1% 62.5mW 厚膜电阻
Supplier Part
C25744
Manufacturer
UNI-ROYAL(厚声)
Manufacturer Part
0402WGF1002TCE
Supplier Footprint
0402
JLCPCB Part Class
Basic Part
Datasheet
https://item.szlcsc.com/datasheet/0402WGF1002TCE/26487.html
Supplier
LCSC
Add into BOM
yes
3D Model Title
R0402_L1.0-W0.5-H0.4
Type
厚膜电阻
Value
10kΩ
Tolerance
±1%
Power(Watts)
62.5mW
Voltage-Supply(Max)
50V
Temperature Coefficient
±100ppm/℃
Operating Temperature
-55℃~+155℃
Name
10kΩ
Description
电阻类型:厚膜电阻;阻值:10kΩ;精度:±1%;功率:62.5mW;工作电压:50V;温度系数:±100ppm/℃;
Device
0402WGF1002TCE
Unique ID
gge109
Reuse Block

Group ID

Channel ID
$1I181
PCB Layer
TopLayer
Convert to PCB
yes

*
]
[
DESIGNATOR
R15
FOOTPRINT
R0402
PARTTYPE
0402WGF1002TCE
DESCRIPTION
电阻类型:厚膜电阻;阻值:10kΩ;精度:±1%;功率:62.5mW;工作电压:50V;温度系数:±100ppm/℃;
Component Kind
Standard
Footprint
R0402
Designator
R15
LCSC Part Name
10kΩ ±1% 62.5mW 厚膜电阻
Supplier Part
C25744
Manufacturer
UNI-ROYAL(厚声)
Manufacturer Part
0402WGF1002TCE
Supplier Footprint
0402
JLCPCB Part Class
Basic Part
Datasheet
https://item.szlcsc.com/datasheet/0402WGF1002TCE/26487.html
Supplier
LCSC
Add into BOM
yes
3D Model Title
R0402_L1.0-W0.5-H0.4
Type
厚膜电阻
Value
10kΩ
Tolerance
±1%
Power(Watts)
62.5mW
Voltage-Supply(Max)
50V
Temperature Coefficient
±100ppm/℃
Operating Temperature
-55℃~+155℃
Name
10kΩ
Description
电阻类型:厚膜电阻;阻值:10kΩ;精度:±1%;功率:62.5mW;工作电压:50V;温度系数:±100ppm/℃;
Device
0402WGF1002TCE
Unique ID
gge110
Reuse Block

Group ID

Channel ID
$1I182
PCB Layer
TopLayer
Convert to PCB
yes

*
]
[
DESIGNATOR
D3
FOOTPRINT
SOD-123FL_L2.7-W1.8-LS3.8-RD
PARTTYPE
SMF5.0A_C19077497
DESCRIPTION
极性:单向;反向截止电压(Vrwm):5V;钳位电压:9.2V;峰值脉冲电流(Ipp):21.7A@10/1000us;峰值脉冲功率(Ppp):200W@10/1000us;击穿电压:7V;
Component Kind
Standard
Footprint
SOD-123FL_L2.7-W1.8-LS3.8-RD
Designator
D3
LCSC Part Name
单向TVS 5V截止 峰值浪涌电流：21.7A@10/1000us
Supplier Part
C19077497
Manufacturer
R+O(宏嘉诚)
Manufacturer Part
SMF5.0A
Supplier Footprint
SOD-123FL
JLCPCB Part Class
Extended Part
Datasheet
https://item.szlcsc.com/datasheet/SMF5.0A/20275582.html
Supplier
LCSC
Add into BOM
yes
3D Model Title
SOD-123FL_L2.8-W1.8-H1.1-LS3.6
Polarity
单向
Reverse Stand-Off Voltage (Vrwm)
5V
Clamping Voltage
9.2V
Peak Pulse Current (Ipp)
21.7A@10/1000us
Peak Pulse Power Dissipation (Ppp)
200W@10/1000us
Voltage - Breakdown
7V
Reverse Leakage Current (Ir)
400uA
Number of Channels
单路
Operating Temperature
-55℃~+150℃
level of protection
IEC 61000-4-2
Type
TVS
Junction Capacitance
-
Name
SMF5.0A
Description
极性:单向;反向截止电压(Vrwm):5V;钳位电压:9.2V;峰值脉冲电流(Ipp):21.7A@10/1000us;峰值脉冲功率(Ppp):200W@10/1000us;击穿电压:7V;
Device
SMF5.0A_C19077497
Unique ID
gge108
Reuse Block

Group ID

Channel ID
$1I180
PCB Layer
TopLayer
Convert to PCB
yes

*
]
[
DESIGNATOR
C24
FOOTPRINT
C0805
PARTTYPE
CL21A226MAQNNNE
DESCRIPTION
容值:22uF;精度:±20%;额定电压:25V;温度系数:X5R;
Component Kind
Standard
Footprint
C0805
Designator
C24
LCSC Part Name
22uF ±20% 25V
Supplier Part
C45783
Manufacturer
SAMSUNG(三星)
Manufacturer Part
CL21A226MAQNNNE
Supplier Footprint
0805
JLCPCB Part Class
Basic Part
Datasheet
https://item.szlcsc.com/datasheet/CL21A226MAQNNNE/46786.html
Supplier
LCSC
Add into BOM
yes
3D Model Title
C0805_L2.0-W1.3-H1.3
Value
22uF
Tolerance
±20%
Voltage Rating
25V
Temperature Coefficient
X5R
Name
22uF
Description
容值:22uF;精度:±20%;额定电压:25V;温度系数:X5R;
Device
CL21A226MAQNNNE
Unique ID
gge111
Reuse Block

Group ID

Channel ID
$1I186
PCB Layer
TopLayer
Convert to PCB
yes

*
]
[
DESIGNATOR
C2
FOOTPRINT
C0402
PARTTYPE
CL05A106MQ5NUNC
DESCRIPTION
容值:10uF;精度:±20%;额定电压:6.3V;温度系数:X5R;
Component Kind
Standard
Footprint
C0402
Designator
C2
LCSC Part Name
10uF ±20% 6.3V
Supplier Part
C15525
Manufacturer
SAMSUNG(三星)
Manufacturer Part
CL05A106MQ5NUNC
Supplier Footprint
0402
JLCPCB Part Class
Basic Part
Datasheet
https://item.szlcsc.com/datasheet/CL05A106MQ5NUNC/16204.html
Supplier
LCSC
Add into BOM
yes
3D Model Title
C0402_L1.0-W0.5-H0.5
Value
10uF
Tolerance
±20%
Voltage Rating
6.3V
Temperature Coefficient
X5R
Name
10uF
Description
容值:10uF;精度:±20%;额定电压:6.3V;温度系数:X5R;
Device
CL05A106MQ5NUNC
Unique ID
gge112
Reuse Block

Group ID

Channel ID
$1I188
PCB Layer
TopLayer
Convert to PCB
yes

*
]
(
GND 
BOOT-1 TS-1088-AR02016-1 Passive 
C1-2 CL05B104KB54PNC-2 Passive 
C3-1 CL10A106MA8NRNC-1 Passive 
C4-1 CL05A105KA5NQNC-1 Passive 
C5-1 CL10A225KO8NNNC-1 Passive 
C6-1 CL10A225KO8NNNC-1 Passive 
C7-1 CC0603KRX7R9BB104-1 Passive 
C8-1 CL10A106MA8NRNC-1 Passive 
C9-2 CL10A106MA8NRNC-2 Passive 
C10-2 CL05B104KO5NNNC-2 Passive 
C11-2 CL10A106MA8NRNC-2 Passive 
C12-2 CL05B104KO5NNNC-2 Passive 
C13-2 CL05B104KO5NNNC-2 Passive 
C14-2 CC0603KRX7R9BB104-2 Passive 
C15-2 CL05B104KB54PNC-2 Passive 
C16-2 0402CG220J500NT-2 Passive 
C17-2 0402CG220J500NT-2 Passive 
C18-2 CL05B104KB54PNC-2 Passive 
C19-2 CL05B104KB54PNC-2 Passive 
C20-2 CL05B104KB54PNC-2 Passive 
C21-2 CL05B104KB54PNC-2 Passive 
C22-2 CL05B104KB54PNC-2 Passive 
J1-A1B12 TYPE-C 16PIN 2MD(073)-A1B12 Passive 
J1-B1A12 TYPE-C 16PIN 2MD(073)-B1A12 Passive 
J2-1 B8B-XH-AM(LF)(SN)-1 Passive 
J3-2 B2B-XH-A(LF)(SN)-2 Passive 
J6-3 B4B-XH-A(LF)(SN)-3 Passive 
R6-2 0402WGF5101TCE-2 Passive 
R7-1 0402WGF5101TCE-1 Passive 
R11-2 0402WGF1002TCE-2 Passive 
R12-2 0402WGF1002TCE-2 Passive 
RESET-2 TS-1088-AR02016-2 Passive 
SPK1-3 FS-1340-3 Passive 
SPK1-4 FS-1340-4 Passive 
U1-57 ESP32-S3FH4R2-57 Passive 
U2-1 ME6211A33PG-N-1 Passive 
U3-3 MAX98357AETE+T-3 Passive 
U3-11 MAX98357AETE+T-11 Passive 
U3-15 MAX98357AETE+T-15 Passive 
U3-17 MAX98357AETE+T-17 Passive 
U4-9 IP5306-9 Passive 
U5-5 LIS3DHTR-5 Passive 
U5-7 LIS3DHTR-7 Passive 
U5-10 LIS3DHTR-10 Passive 
U5-12 LIS3DHTR-12 Passive 
X1-2 TXM40M0004252HBCEO00T-2 Passive 
X1-4 TXM40M0004252HBCEO00T-4 Passive 
R13-2 0402WGF4702TCE-2 Passive 
C23-2 CL10A106KP8NNNC-2 Passive 
C25-1 CL10A106KP8NNNC-1 Passive 
R15-2 0402WGF1002TCE-2 Passive 
D3-2 SMF5.0A_C19077497-2 Passive 
C24-2 CL21A226MAQNNNE-2 Passive 
C2-1 CL05A106MQ5NUNC-1 Passive 
)
(
$1N183 
BOOT-2 TS-1088-AR02016-2 Passive 
R1-2 0402WGF1002TCE-2 Passive 
U1-5 ESP32-S3FH4R2-5 Passive 
)
(
3V3 
C1-1 CL05B104KB54PNC-1 Passive 
C3-2 CL10A106MA8NRNC-2 Passive 
C6-2 CL10A225KO8NNNC-2 Passive 
C7-2 CC0603KRX7R9BB104-2 Passive 
C8-2 CL10A106MA8NRNC-2 Passive 
C10-1 CL05B104KO5NNNC-1 Passive 
C11-1 CL10A106MA8NRNC-1 Passive 
C12-1 CL05B104KO5NNNC-1 Passive 
C13-1 CL05B104KO5NNNC-1 Passive 
C15-1 CL05B104KB54PNC-1 Passive 
C18-1 CL05B104KB54PNC-1 Passive 
C21-1 CL05B104KB54PNC-1 Passive 
C22-1 CL05B104KB54PNC-1 Passive 
D1-1 KT-0603R-1 Passive 
J2-2 B8B-XH-AM(LF)(SN)-2 Passive 
J2-8 B8B-XH-AM(LF)(SN)-8 Passive 
J6-4 B4B-XH-A(LF)(SN)-4 Passive 
L2-2 BLM18PG121SN1D-2 Passive 
R1-1 0402WGF1002TCE-1 Passive 
R3-1 0402WGF4701TCE-1 Passive 
R4-1 0402WGF4701TCE-1 Passive 
R5-2 0402WGF1002TCE-2 Passive 
U1-2 ESP32-S3FH4R2-2 Passive 
U1-3 ESP32-S3FH4R2-3 Passive 
U1-20 ESP32-S3FH4R2-20 Passive 
U1-29 ESP32-S3FH4R2-29 Passive 
U1-46 ESP32-S3FH4R2-46 Passive 
U2-3 ME6211A33PG-N-3 Passive 
U3-2 MAX98357AETE+T-2 Passive 
U3-7 MAX98357AETE+T-7 Passive 
U3-8 MAX98357AETE+T-8 Passive 
U5-1 LIS3DHTR-1 Passive 
U5-8 LIS3DHTR-8 Passive 
U5-14 LIS3DHTR-14 Passive 
)
(
RESET 
C4-2 CL05A105KA5NQNC-2 Passive 
R5-1 0402WGF1002TCE-1 Passive 
RESET-1 TS-1088-AR02016-1 Passive 
U1-4 ESP32-S3FH4R2-4 Passive 
)
(
BAT 
C5-2 CL10A225KO8NNNC-2 Passive 
J3-1 B2B-XH-A(LF)(SN)-1 Passive 
U2-2 ME6211A33PG-N-2 Passive 
U4-6 IP5306-6 Passive 
C25-2 CL10A106KP8NNNC-2 Passive 
R14-2 0402WGF1002TCE-2 Passive 
)
(
VBUS 
C9-1 CL10A106MA8NRNC-1 Passive 
C14-1 CC0603KRX7R9BB104-1 Passive 
U4-1 IP5306-1 Passive 
R8-1 0603WAF0000T5E-1 Passive 
C23-1 CL10A106KP8NNNC-1 Passive 
)
(
$1N222 
C16-1 0402CG220J500NT-1 Passive 
U1-53 ESP32-S3FH4R2-53 Passive 
X1-3 TXM40M0004252HBCEO00T-3 Passive 
)
(
$1N227 
C17-1 0402CG220J500NT-1 Passive 
L1-2 LQW15AN24NG00D-2 Passive 
X1-1 TXM40M0004252HBCEO00T-1 Passive 
)
(
$1N236 
C19-1 CL05B104KB54PNC-1 Passive 
C20-1 CL05B104KB54PNC-1 Passive 
L2-1 BLM18PG121SN1D-1 Passive 
U1-55 ESP32-S3FH4R2-55 Passive 
U1-56 ESP32-S3FH4R2-56 Passive 
C2-2 CL05A106MQ5NUNC-2 Passive 
)
(
$1N257 
D1-2 KT-0603R-2 Passive 
R2-1 0402WGF1001TCE-1 Passive 
)
(
$1N173 
J1-A4B9 TYPE-C 16PIN 2MD(073)-A4B9 Passive 
J1-B4A9 TYPE-C 16PIN 2MD(073)-B4A9 Passive 
R8-2 0603WAF0000T5E-2 Passive 
D3-1 SMF5.0A_C19077497-1 Passive 
)
(
$1N152 
J1-A5 TYPE-C 16PIN 2MD(073)-A5 Passive 
R6-1 0402WGF5101TCE-1 Passive 
)
(
USBDN 
J1-B7 TYPE-C 16PIN 2MD(073)-B7 Passive 
J1-A7 TYPE-C 16PIN 2MD(073)-A7 Passive 
R9-1 0402WGF220JTCE-1 Passive 
)
(
USBDP 
J1-A6 TYPE-C 16PIN 2MD(073)-A6 Passive 
J1-B6 TYPE-C 16PIN 2MD(073)-B6 Passive 
R10-1 0402WGF220JTCE-1 Passive 
)
(
$1N95 
J1-B5 TYPE-C 16PIN 2MD(073)-B5 Passive 
R7-2 0402WGF5101TCE-2 Passive 
)
(
LCDCLK 
J2-3 B8B-XH-AM(LF)(SN)-3 Passive 
U1-17 ESP32-S3FH4R2-17 Passive 
)
(
LCDMOSI 
J2-4 B8B-XH-AM(LF)(SN)-4 Passive 
U1-16 ESP32-S3FH4R2-16 Passive 
)
(
LCDRST 
J2-5 B8B-XH-AM(LF)(SN)-5 Passive 
U1-13 ESP32-S3FH4R2-13 Passive 
)
(
LCDDC 
J2-6 B8B-XH-AM(LF)(SN)-6 Passive 
U1-14 ESP32-S3FH4R2-14 Passive 
)
(
LCDCS 
J2-7 B8B-XH-AM(LF)(SN)-7 Passive 
U1-15 ESP32-S3FH4R2-15 Passive 
)
(
TOUCHRFACE 
J4-1 B3B-XH-A(LF)(SN)-1 Passive 
U1-11 ESP32-S3FH4R2-11 Passive 
)
(
TOUCHLFACE 
J4-2 B3B-XH-A(LF)(SN)-2 Passive 
U1-7 ESP32-S3FH4R2-7 Passive 
)
(
TOUCHHEAD 
J4-3 B3B-XH-A(LF)(SN)-3 Passive 
U1-6 ESP32-S3FH4R2-6 Passive 
)
(
TXD0 
J6-1 B4B-XH-A(LF)(SN)-1 Passive 
U1-49 ESP32-S3FH4R2-49 Passive 
)
(
RXD0 
J6-2 B4B-XH-A(LF)(SN)-2 Passive 
U1-50 ESP32-S3FH4R2-50 Passive 
)
(
$1N221 
L1-1 LQW15AN24NG00D-1 Passive 
U1-54 ESP32-S3FH4R2-54 Passive 
)
(
SW 
L3-1 FXL0420-1R0-M-1 Passive 
U4-7 IP5306-7 Passive 
)
(
VOUT 
L3-2 FXL0420-1R0-M-2 Passive 
U4-8 IP5306-8 Passive 
C24-1 CL21A226MAQNNNE-1 Passive 
)
(
$1N258 
R2-2 0402WGF1001TCE-2 Passive 
U4-2 IP5306-2 Passive 
)
(
ACCELSCL 
R3-2 0402WGF4701TCE-2 Passive 
U1-23 ESP32-S3FH4R2-23 Passive 
U5-4 LIS3DHTR-4 Passive 
)
(
ACCELSDA 
R4-2 0402WGF4701TCE-2 Passive 
U1-24 ESP32-S3FH4R2-24 Passive 
U5-6 LIS3DHTR-6 Passive 
)
(
$1N200 
R9-2 0402WGF220JTCE-2 Passive 
U1-25 ESP32-S3FH4R2-25 Passive 
)
(
$1N199 
R10-2 0402WGF220JTCE-2 Passive 
U1-26 ESP32-S3FH4R2-26 Passive 
)
(
$1N215 
R11-1 0402WGF1002TCE-1 Passive 
U1-52 ESP32-S3FH4R2-52 Passive 
)
(
$1N216 
R12-1 0402WGF1002TCE-1 Passive 
U1-51 ESP32-S3FH4R2-51 Passive 
)
(
SPKP 
SPK1-1 FS-1340-1 Passive 
U3-9 MAX98357AETE+T-9 Passive 
)
(
SPKN 
SPK1-2 FS-1340-2 Passive 
U3-10 MAX98357AETE+T-10 Passive 
)
(
I2SBCLK 
U1-9 ESP32-S3FH4R2-9 Passive 
U3-16 MAX98357AETE+T-16 Passive 
)
(
I2SWS 
U1-10 ESP32-S3FH4R2-10 Passive 
U3-14 MAX98357AETE+T-14 Passive 
)
(
AMPDIN 
U1-12 ESP32-S3FH4R2-12 Passive 
U3-1 MAX98357AETE+T-1 Passive 
)
(
AMPSDMODE 
U1-18 ESP32-S3FH4R2-18 Passive 
U3-4 MAX98357AETE+T-4 Passive 
R13-1 0402WGF4702TCE-1 Passive 
)
(
BATADC 
U1-19 ESP32-S3FH4R2-19 Passive 
R14-1 0402WGF1002TCE-1 Passive 
R15-1 0402WGF1002TCE-1 Passive 
)
(
ACCELINT1 
U1-27 ESP32-S3FH4R2-27 Passive 
U5-11 LIS3DHTR-11 Passive 
)
